| ECC1C 145-944-00

Temperature Manager

Temperature Manager system ID: 0x22

The temperature manager system provides information about the actuator and the driver temperatures. Temperature limits can be set explicitly to prevent overheating.

### Register Map:

Address | Name | Default | Description | Type | Access
--- | --- | --- | --- | --- | ---
0x2200 | Device temperature | N/A | Degrees Celsius | float | read only
0x2201 | Device temperature threshold | 80 | Degrees Celsius. If this threshold is reached the output of the driver is disabled to cool down. Temperature has to fall by 10 degrees so that the output is enabled again | float | read write
0x2202 | Output Stage (MAX31875) temperature | N/A | Degrees Celsius | float | read only
0x2203 | Output Stage (MAX31875) temp. threshold | 110 | Degrees Celsius. If this threshold is reached the output of the driver is disabled to cool down. Temperature has to fall by 10 degrees so that the output is enabled again | float | read write
0x2204 | Power Supply (MCU) temperature | N/A | Degrees Celsius | float | read only
0x2205 | Power Supply (MCU) temperature threshold | 130 | Degrees Celsius. If this threshold is reached the output of the driver is disabled to cool down. Temperature has to fall by 10 degrees so that the output is enabled again | float | read write