| ECC1C 145-944-00

Static Input

Static Input system ID: 0x50

The static input stage system belongs to the input stage systems of the Signal Flow and is the one which is by factory default activated at start up. With this system the user can set constant values as input to the signal flow.

### Register Map:

Address | Name | Default Value | Description | Type | Access
--- | --- | --- | --- | --- | ---
0x5000 | Current static input | 0.0 | Static input in amperes. Range is from -0.318 to 0.318 | float | read write
0x5001 | not used |  |  | float | read write
0x5002 | not used | 0.0 |  | float | read write
0x5003 | Active static input type | 0 | Determined by active control stage system | Unit Type | read only
0x5004 | FP static input | 0.0 | Static input in diopters | float | read write