| ECC1C 145-944-00

Signal Flow Manager

Signal Flow Manager system ID: 0x40

The Signal Flow Manager is providing registers to set up signal flow systems for each stage. The specific register address depends on the index of signal flow stage and the index of the channel. The general address of the Signal Flow Manager register controlling stage with index S in channel with index C is:

    S + 5*C

Attention
  Stages and channels are indexed from 0.

The Signal Flow consists of five stages.

Signal Flow Stage | Index
--- | ---
Input stage | 0
Input conditioning stage | 1
Control stage | 2
Output conditioning stage | 3
Output stage | 4

For example, the register for the control stage (index 2) of the second channel (index 1) is 2 + 5*1 = 7

### Register Map:

Address | Name | Default Value | Description | Type | Access
--- | --- | --- | --- | --- | ---
0x4000 | Active input system of channel one | 0x50 | System ID is expected | uint32 | read write
0x4002 | Active control system of channel one | 0xB0 | System ID is expected | uint32 | read write

### Examples:

To activate the signal generator system for channel one, set to register with address 0x4000 the value 0x61.