| ECC1C 145-944-00

Vector Pattern Unit

Vector Pattern Unit system ID: 0x68

The Vector Pattern Unit system is an input stage system that can used to propagate arbitrary vector values set by the user as input to the Signal Flow. The values must be saved in the Vector Pattern Memory. The Vector Pattern system has to be activated through the Signal Flow Manager. Unit type has to match to the configured control mode.

### Register Map:

Address | Name | Default Value | Description | Type | Access
--- | --- | --- | --- | --- | ---
0x6800 | Unit type | 0 |  | Unit Type | read write
0x6801 | Run | false | Turn Vector Pattern Unit on/off | boolean | read write
0x6802 | Start | 0 | Index of first desired point in Vector Pattern Memory | uint32 | read write
0x6803 | End | 0 | Index after last desired point in Vector Pattern Memory | uint32 | read write
0x6804 | Sample rate | 20000 | Sample rate at which the Vector Pattern unit samples the vector in the Vector Pattern Memory | float | read write
0x6805 | Minimum sampling rate |  | In Hz | float | read only
0x6806 | Maximum sampling rate | 20000 | In Hz | float | read only
0x6807 | Cycles | -1 | Number of cycles to be generated. Run flag is turned off after completion. Negative value corresponds to infinite looping | int32 | read write
0x6808 | External trigger | 0 | Vector Pattern Unit can be synchronised with external signal (0=disabled, 1=rising/falling edge, 2=rising edge trigger) | uint32 | read write
0x6809 | Output | N/A | Output of the vector pattern unit | float | read only