| ECC1C 145-944-00

Snapshot Manager

Snapshot system ID: 0x27

A system that supports saving and loading firmware configurations.

### Register Map:

Address | Name | Default Value | Description | Type | Access
--- | --- | --- | --- | --- | ---
0x2700 | Snapshot capacity | 1 | Number of available snapshot slots, read-only | uint32 | read only
0x2701 | Default snapshot | 0 | Snapshot to load on system startup | uint32 | read write
0x2702 | Error system | 0 | ID of system which caused the last snapshot error | uint8 | read only
0x2703 | Error register | 0 | ID of register which caused the last snapshot error | uint8 | read only
0x2704 | Error value | 0 | Value which caused the last snapshot error | uint32 | read only