| ECC1C 145-944-00

Vector Pattern Memory

Vector Pattern Memory system ID: 0x26

Vector Pattern Memory system is a memory that is shared by all Vector Pattern Unit systems of all channels.

### Register Map:

Address | Name | Default Value | Description | Type | Access
--- | --- | --- | --- | --- | ---
0x2600 | Vector pattern data valid | false | Writing 0 to this register causes the firmware to write the vector pattern memory contents (RAM) to the flash memory | boolean | read write

### Vector Map:

Address | Name | Default Value | Description | Type | Access
--- | --- | --- | --- | --- | ---
0x2600 | Vector pattern data | N/A | Contents of the Vector Pattern Memory. Only addressable by units of uint32 (all indices and sizes must be divisible by 4) | uint32[5000] | read write

Attention
  Vectors have their own address space.