ICC C# SDK

Loading...
Searching...
No Matches
ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController Member List

This is the complete list of members for ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController, including all inherited members.

AnalogInput | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
ArbitraryVector | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
BoardEeprom | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
ChangeActiveSystem(EChannel channel, EInputSignalStageSystem selectedInputStageSystem) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
ChangeModeToPro() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
ChangeModeToSimple() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
Connect(int port) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
Connect(string ipAddress, int port) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
ControlModeStage | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
DeviceEeprom | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
Disconnect(bool cleanUp) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
EnableSensorReadout(bool enable) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetAdcI(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetAdcV(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetAmplitude(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetAnalogActiveInputType(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetAnalogIn(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetAnalogInputCurrentMax(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetAnalogInputCurrentMin(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetAnalogInputDiopterMax(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetAnalogInputDiopterMin(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetAnalogInputExtrapolation(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetAnalogInputType(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetAutoConfig() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetBoardFirmwareBranch() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetBoardFirmwareBuildVersion() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetBoardFirmwareId() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetBoardFirmwareMajorVersion() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetBoardFirmwareMinorVersion() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetBoardFirmwareRevisionVersion() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetBoardFirmwareType() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetBoardOutputTemperature() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetBoardOutputTemperatureThreshold() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetBoardPowerTemperature() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetBoardPowerTemperatureThreshold() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetBytes(EChannel channel, int index, int length) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetConnectedDeviceTypes() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetCurrent(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetDeviceDetectChannelMask() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetDeviceEepromSize(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetDeviceStatus() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetDeviceTemperature(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetDeviceTemperatureThreshold(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetDeviceType(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetDevPower(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetDiopter(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetDutyCycles(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetEepromActiveChannel() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetEepromSubVersion(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetEepromVersion(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetElectronicSerialNumber() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetExternalTriggerDivider(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetExternalTriggerGpio(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetExternalTriggerOffset(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetFirmwareSerialNumber() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetFrequency(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetFrontEndPowerState() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetFrontEndVoltage() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetGitHeadSha1() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetGPIODirection() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetGPIOState() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetI2CList(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetIin() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetInputSignalVectorPatternValues(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetLensCompensationOutputCurrent(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetLensCompensationOutputDiopter(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetLoggedRegisterAddress(int registerNumber) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetLoggerMaximumSamplingRate() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetLoggerMinimumSamplingRate() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetLoggerSamplingRate() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetMaximumSamplingRate(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetMaxNegativeCurrent(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetMaxPositiveCurrent(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetMinimumAndMaximumCurrent(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetMinimumSamplingRate(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetNormalisedHallSensor(ESensor sensor) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetOqcResult(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetOutputStageCurrentLimit(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetOutputStageEnabled(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetOutputStageOutputCurrent(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetOutputStagePwmFrequency() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetOutputStageSensorOutput(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetPartConfiguration(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetPartConfigurationVersion(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetPhaseDelay(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetPhaseDelayDegrees(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetPinAvg() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetProductionTimeStamp(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetProductSerialNumberOnChannel(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetProductTypeOnChannel(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetResistance(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetSampleRate(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetScale(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetShape(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetSignalGeneratorValues(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetSmartStepManagerFilterActivated(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetStageOutput(ESignalFlowPath path, EStage stage, EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetTransitionRate(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetUfe() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetUin() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetUnitlessValue(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetValue(int registerId) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetVector(int registerId, int index, int count) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetVectorValues(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GetWcState() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
GoToDfuMode() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
HallFeedback | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
ICC4cPwmSdkDeviceController(bool isEthernet=false) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
InputConditioningStage | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
InputStage | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
IsConnected() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
LensCompensation | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
LoadSnapshot(int snapshotNumber) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
LockDeviceEepromWriting(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
LoggerFeatures | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
MiscFeatures | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
OffsetAndScale | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
OutputStage | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
ReadLoggerRegisterLog(int registerNumber, int startIndex, int numberOfLoggedValues) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
ReadNumberOfAvailableSnapshots() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
ReadSnapshotManagerErrorRegisterId() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
ReadSnapshotManagerErrorSystemId() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
ReadSnapshotManagerErrorValue() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
ReadStartupSnapshotNumber() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
Reconnect() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
ReparseDeviceEeprom(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
ResetErrorFlags() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
ResetFirmware() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SaveSnapshot(int snapshotNumber) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SensorTransformMatrix(EChannel channel, float[] matrix) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetActiveSystem(EIcc4cControlModeSystems controlModeSystem, EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetAmplitude(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetAnalogInputCurrentMax(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetAnalogInputCurrentMin(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetAnalogInputDiopterMax(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetAnalogInputDiopterMin(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetAnalogInputExtrapolation(EChannel channel, EExtrapolationType extrapolation) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetAnalogInputType(EChannel channel, EICC4cPwmUnitType type) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetAnalogInputValuePoints(EChannel channel, float[] values) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetAnalogInputVoltagePoints(EChannel channel, float[] voltages) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetAutoConfig(EAutoConfig eAutoConfig) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetBoardOutputTemperatureThreshold(float temperatureThreshold) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetBoardPowerTemperatureThreshold(float temperatureThreshold) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetBytes(EChannel channel, int index, byte[] inputBytes) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetCurrent(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetDefaultState(int value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetDeviceDetectChannelMask(int detectMask) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetDeviceTemperatureThreshold(EChannel channel, float temperatureThreshold) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetDevPower(EChannel channel, int power) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetDiopter(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetDutyCycles(EChannel channel, float dutyCycles) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetEepromActiveChannel(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetExternalTriggerDivider(EChannel channel, int divider) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetExternalTriggerGpio(EChannel channel, EExternalTriggerGpiox gpio) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetExternalTriggerOffset(EChannel channel, int divider) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetFontEndPowerState(bool state) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetFrequency(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetFrontEndVoltage(float frontEndVoltage) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetGpioDirection(int value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetGpioState(int value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetInputSignalVectorPatternValues(EChannel channel, IList< float > values, int requiredStartIndex, bool isSecondPart) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetLinearizationCoefficients(ESensor sensor, float c, float d1, float d2, float d3, float d4, float e) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetLoggedRegisterAddress(int registerNumber, ushort registerAddress) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetLoggerSamplingRate(float samplingRate) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetOutputConditioningStageSystem(EChannel channel, EOutputConditioningStageSystem filter) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetOutputStageCurrentLimit(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetOutputStageEnabled(EChannel channel, bool enabled) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetOutputStagePwmFrequency(EPwmFrequency frequency) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetPhaseDelay(EChannel channel, float phaseDelay) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetPhaseDelayDegrees(EChannel channel, float phaseDelay) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetPidAsControlMode(EChannel channel, int enabled) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetPidFilterCutOffFrequencyOnChannel(EChannel channel, float frequency) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetPidGainsOnChannel(EChannel channel, float kp, float ki, float kd) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetPidMinMaxOutputFeedbackOnChannel(EChannel channel, float min, float max) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetSampleRate(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetScale(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetShape(EChannel channel, ESignalGeneratorShape shape) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetSignalGeneratorValues(EChannel channel, SignalGeneratorParametersDto parameters) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetSmartStepManagerFilter(EChannel channel, bool isEnabled) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetTransitionRate(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetUnitlessValue(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetUnitType(EChannel channel, EICC4cPwmUnitType unit) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetValue(int registerId, ValueType value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetVector(int registerId, int index, byte[] vector) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetVectorValues(EChannel channel, float[] values, int startIndex=0) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SetWcState(int state) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SignalFlowManager | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SignalGenerator | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SmartStepManager | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SnapshotManager | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
StartLogger() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
StaticValue | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
Status | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
StopLogger() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SwitchArbitraryVector(EChannel channel, bool running) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SwitchRunning(EChannel channel, bool enable) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
TemperatureManager | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
UnlockDeviceEepromWriting(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
VectorPatternMemory | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
WriteStartupSnapshotNumber(int snapshotNumber) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |