ICC-4c C# SDK

ICC4cPwmSdk.Device.Ecc1cSdkDeviceController Member List

This is the complete list of members for ICC4cPwmSdk.Device.Ecc1cSdkDeviceController, including all inherited members.

ArbitraryVector (defined in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController |
ChangeActiveSystem(EInputSignalStageSystem selectedInputStageSystem) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
ChangeModeToPro() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
ChangeModeToSimple() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
Connect(int port) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
ControlModeStage (defined in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController |
DeviceEeprom (defined in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController |
Disconnect() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
Ecc1cSdkDeviceController() (defined in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetAdcI() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetAdcV() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetAmplitude() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetAnalogIn() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetAutoConfig() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetBoardFirmwareBranch() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetBoardFirmwareBuildVersion() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetBoardFirmwareId() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetBoardFirmwareMajorVersion() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetBoardFirmwareMinorVersion() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetBoardFirmwareRevisionVersion() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetBoardFirmwareType() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetBoardOutputTemperature() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetBoardOutputTemperatureThreshold() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetBoardPowerTemperature() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetBoardPowerTemperatureThreshold() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetBytes(int index, int length) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetCurrent() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetDeviceEepromSize() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetDeviceStatus() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetDeviceTemperature() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetDeviceTemperatureThreshold() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetDeviceType() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetDevPower() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetDiopter() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetDutyCycles() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetEepromActiveChannel() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetEepromSubVersion() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetEepromVersion() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetElectronicSerialNumber() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetFirmwareSerialNumber() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetFrequency() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetFrontEndPowerState() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetFrontEndVoltage() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetGitHeadSha1() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetGPIOState() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetI2CList() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetIin() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetLensCompensationOutputCurrent() (defined in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetLensSerialNumber() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetLensType() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetMaximumSamplingRate() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetMaxNegativeCurrent() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetMaxPositiveCurrent() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetMinimumSamplingRate() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetOqcResult() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetOutputStageEnabled() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetOutputStagePwmFrequency() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetPartConfiguration() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetPartConfigurationVersion() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetPhaseDelay() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetProductionTimeStamp() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetResistance() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetSampleRate() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetScale() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetShape() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetSignalGeneratorValues() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetUfe() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetUin() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GetVectorValues() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
GoToDfuMode() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
InputConditioningStage (defined in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController |
InputStage (defined in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController |
IsConnected() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
LensCompensation (defined in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController |
LockDeviceEepromWriting() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
MiscFeatures (defined in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController |
OffsetAndScale (defined in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController |
OutputStage (defined in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController |
Reconnect() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
ReparseDeviceEeprom() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
ResetErrorFlags() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
ResetFirmware() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetActiveSystem(EIcc4cControlModeSystems controlModeSystem) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetAmplitude(float value) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetAutoConfig(EAutoConfig eAutoConfig) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetBoardOutputTemperatureThreshold(float temperatureThreshold) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetBoardPowerTemperatureThreshold(float temperatureThreshold) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetBytes(int index, byte[] inputBytes) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetCurrent(float value) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetDeviceTemperatureThreshold(float temperatureThreshold) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetDevPower(int power) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetDiopter(float value) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetDutyCycles(float dutyCycles) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetFontEndPowerState(bool state) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetFrequency(float value) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetFrontEndVoltage(float frontEndVoltage) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetGpioState(int value) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetOutputStageEnabled(bool enabled) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetOutputStagePwmFrequency(EPwmFrequency frequency) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetPhaseDelay(float phaseDelay) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetSampleRate(float value) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetScale(float value) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetShape(ESignalGeneratorShape shape) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetSignalGeneratorValues(SignalGeneratorParametersDto parameters) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetUnitType(EICC4cPwmUnitType unit) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SetVectorValues(float[] values, int startIndex=0) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SignalFlowManager (defined in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController |
SignalGenerator (defined in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController |
StaticValue (defined in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController |
Status (defined in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController |
SwitchArbitraryVector(bool running) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
SwitchRunning(bool enable) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline
TemperatureManager (defined in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController) | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController |
UnlockDeviceEepromWriting() | ICC4cPwmSdk.Device.Ecc1cSdkDeviceController | inline