ICC-4c C# SDK

ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController Member List

This is the complete list of members for ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController, including all inherited members.

ArbitraryVector (defined in ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
ChangeActiveSystem(EChannel channel, EInputSignalStageSystem selectedInputStageSystem) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
ChangeModeToPro() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
ChangeModeToSimple() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
Connect(int port) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
Connect(string ipAddress, int port) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
ControlModeStage (defined in ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
DeviceEeprom (defined in ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
Disconnect() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetAdcI(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetAdcV(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetAmplitude(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetAnalogIn(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetAutoConfig() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetBoardFirmwareBranch() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetBoardFirmwareBuildVersion() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetBoardFirmwareId() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetBoardFirmwareMajorVersion() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetBoardFirmwareMinorVersion() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetBoardFirmwareRevisionVersion() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetBoardFirmwareType() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetBoardOutputTemperature() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetBoardOutputTemperatureThreshold() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetBoardPowerTemperature() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetBoardPowerTemperatureThreshold() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetBytes(EChannel channel, int index, int length) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetConnectedDeviceTypes() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetCurrent(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetDeviceEepromSize(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetDeviceStatus() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetDeviceTemperature(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetDeviceTemperatureThreshold(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetDeviceType(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetDevPower(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetDiopter(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetDutyCycles(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetEepromActiveChannel() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetEepromSubVersion(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetEepromVersion(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetElectronicSerialNumber() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetFirmwareSerialNumber() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetFrequency(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetFrontEndPowerState() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetFrontEndVoltage() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetGitHeadSha1() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetGPIOState() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetI2CList(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetIin() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetLensCompensationOutputCurrent(EChannel channel) (defined in ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetMaximumSamplingRate(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetMaxNegativeCurrent(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetMaxPositiveCurrent(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetMinimumSamplingRate(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetOqcResult(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetOutputStageEnabled(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetOutputStagePwmFrequency() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetPartConfiguration(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetPartConfigurationVersion(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetPhaseDelay(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetProductionTimeStamp(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetProductSerialNumberOnChannel(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetProductTypeOnChannel(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetResistance(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetSampleRate(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetScale(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetShape(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetSignalGeneratorValues(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetUfe() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetUin() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GetVectorValues(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
GoToDfuMode() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
ICC4cPwmSdkDeviceController(bool isEthernet=false) (defined in ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
InputConditioningStage (defined in ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
InputStage (defined in ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
IsConnected() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
LensCompensation (defined in ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
LockDeviceEepromWriting(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
MiscFeatures (defined in ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
OffsetAndScale (defined in ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
OutputStage (defined in ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
Reconnect() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
ReparseDeviceEeprom(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
ResetErrorFlags() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
ResetFirmware() | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetActiveSystem(EIcc4cControlModeSystems controlModeSystem, EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetAmplitude(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetAutoConfig(EAutoConfig eAutoConfig) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetBoardOutputTemperatureThreshold(float temperatureThreshold) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetBoardPowerTemperatureThreshold(float temperatureThreshold) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetBytes(EChannel channel, int index, byte[] inputBytes) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetCurrent(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetDeviceTemperatureThreshold(EChannel channel, float temperatureThreshold) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetDevPower(EChannel channel, int power) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetDiopter(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetDutyCycles(EChannel channel, float dutyCycles) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetEepromActiveChannel(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetFontEndPowerState(bool state) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetFrequency(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetFrontEndVoltage(float frontEndVoltage) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetGpioState(int value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetOutputStageEnabled(EChannel channel, bool enabled) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetOutputStagePwmFrequency(EPwmFrequency frequency) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetPhaseDelay(EChannel channel, float phaseDelay) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetSampleRate(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetScale(EChannel channel, float value) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetShape(EChannel channel, ESignalGeneratorShape shape) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetSignalGeneratorValues(EChannel channel, SignalGeneratorParametersDto parameters) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetUnitType(EChannel channel, EICC4cPwmUnitType unit) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SetVectorValues(EChannel channel, float[] values, int startIndex=0) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SignalFlowManager (defined in ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SignalGenerator (defined in ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
StaticValue (defined in ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
Status (defined in ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
SwitchArbitraryVector(EChannel channel, bool running) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
SwitchRunning(EChannel channel, bool enable) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline
TemperatureManager (defined in ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController |
UnlockDeviceEepromWriting(EChannel channel) | ICC4cPwmSdk.Device.ICC4cPwmSdkDeviceController | inline