| optoICC

### - s -

- set_accel_resolution() : optoICC.registers.icc_registers.InertialMeasurementUnit
- set_Ain_cal_coef() : optoICC.registers.icc_registers.ICCBoardEEPROM
- set_averaging() : optoICC.registers.icc_registers.HallReadout4Lyra
- set_axis_in_limit_x() : optoICC.registers.icc_registers.SarynControl
- set_axis_in_limit_y() : optoICC.registers.icc_registers.SarynControl
- set_axis_in_limit_z() : optoICC.registers.icc_registers.SarynControl
- set_callback_prescaler() : optoICC.registers.icc_registers.InertialMeasurementUnit
- set_dlpf() : optoICC.registers.icc_registers.InertialMeasurementUnit
- set_gain() : optoICC.registers.icc_registers.HallReadout4Lyra
- set_gyro_resolution() : optoICC.registers.icc_registers.InertialMeasurementUnit
- set_hall_in_limit_ch0() : optoICC.registers.icc_registers.SarynControl
- set_hall_in_limit_ch1() : optoICC.registers.icc_registers.SarynControl
- set_hall_in_limit_ch2() : optoICC.registers.icc_registers.SarynControl
- set_Iin_cal_coef() : optoICC.registers.icc_registers.ICCBoardEEPROM
- set_Int_I_cal_coef() : optoICC.registers.icc_registers.ICCBoardEEPROM
- set_Int_U_cal_coef() : optoICC.registers.icc_registers.ICCBoardEEPROM
- set_max_output_current() : optoICC.registers.icc_registers.SarynControl
- set_meas_delay() : optoICC.registers.icc_registers.HallReadout4Lyra
- set_Out_cal_coef() : optoICC.registers.icc_registers.ICCBoardEEPROM
- set_oversampling() : optoICC.registers.icc_registers.HallReadout4Lyra
- set_pid_coef_ch0() : optoICC.registers.icc_registers.SarynControl
- set_pid_coef_ch1() : optoICC.registers.icc_registers.SarynControl
- set_pid_coef_ch2() : optoICC.registers.icc_registers.SarynControl
- set_pid_coef_os_x() : optoICC.registers.icc_registers.SarynControl
- set_pid_coef_os_y() : optoICC.registers.icc_registers.SarynControl
- set_pid_coef_x() : optoICC.registers.icc_registers.SarynControl
- set_pid_coef_y() : optoICC.registers.icc_registers.SarynControl
- set_pid_coef_z() : optoICC.registers.icc_registers.SarynControl
- set_poly_hall_to_current_ch0() : optoICC.registers.icc_registers.SarynControl
- set_poly_hall_to_current_ch1() : optoICC.registers.icc_registers.SarynControl
- set_poly_hall_to_current_ch2() : optoICC.registers.icc_registers.SarynControl
- set_poly_hall_to_current_x() : optoICC.registers.icc_registers.SarynControl
- set_poly_hall_to_current_y() : optoICC.registers.icc_registers.SarynControl
- set_poly_hall_to_current_z() : optoICC.registers.icc_registers.SarynControl
- set_poly_tf_feedback_hall_to_axis_x() : optoICC.registers.icc_registers.SarynControl
- set_poly_tf_feedback_hall_to_axis_y() : optoICC.registers.icc_registers.SarynControl
- set_poly_tf_feedback_hall_to_axis_z() : optoICC.registers.icc_registers.SarynControl
- set_readout() : optoICC.registers.icc_registers.HallReadout4Lyra
- set_reg() : optoICC.registers.icc_registers.CapacitiveFeedback , optoICC.registers.icc_registers.HallFeedback
- set_resolution() : optoICC.registers.icc_registers.HallReadout4Lyra
- set_t_comp_type() : optoICC.registers.icc_registers.HallFeedback
- set_temp_comp() : optoICC.registers.icc_registers.HallReadout4Lyra
- set_Ufe_cal_coef() : optoICC.registers.icc_registers.ICCBoardEEPROM
- set_Uin_cal_coef() : optoICC.registers.icc_registers.ICCBoardEEPROM
- set_update_freq() : optoICC.registers.icc_registers.SarynControl
- set_x() : optoICC.registers.icc_registers.SarynControl
- set_y() : optoICC.registers.icc_registers.SarynControl
- set_z() : optoICC.registers.icc_registers.SarynControl
- SetAddNoValue() : optoICC.registers.icc_registers.TransformationStage
- SetAddValueOnInput() : optoICC.registers.icc_registers.TransformationStage
- SetAddValueOnOutput() : optoICC.registers.icc_registers.TransformationStage
- setAutoConfig() : optoICC.registers.icc_registers.ICCBoardEEPROM
- SetAutoConfig() : optoICC.registers.icc_registers.ICCMiscFeatures
- SetBoardOutTemperatureThreshold() : optoICC.registers.icc_registers.ICCTemperatureManager
- SetBoardPowTemperatureThreshold() : optoICC.registers.icc_registers.ICCTemperatureManager
- setCalTimestamp() : optoICC.registers.icc_registers.ICCBoardEEPROM
- SetCoeff() : optoICC.registers.icc_registers.LinearizationStage
- SetCoeffs() : optoICC.registers.icc_registers.LinearizationStage
- SetControlMode() : optoICC.icc4c.ICC4cChannel
- setControlSetup() : optoICC.registers.icc_registers.ICCBoardEEPROM
- SetDefaultState() : optoICC.registers.icc_registers.ICCMiscFeatures
- setDevice3V3chanMask() : optoICC.registers.icc_registers.ICCBoardEEPROM
- setDeviceDetectChanMask() : optoICC.registers.icc_registers.ICCBoardEEPROM
- SetDeviceDetectSwitchMask() : optoICC.registers.icc_registers.ICCStatus
- SetDeviceEEPROMactiveChannel() : optoICC.registers.icc_registers.ICCStatus
- SetDevicePower() : optoICC.registers.icc_registers.ICCMiscFeatures
- SetDeviceTemperatureThreshold() : optoICC.registers.icc_registers.ICCDeviceTemperatureManager , optoICC.registers.icc_registers.ICCTemperatureManager
- setDHCP() : optoICC.registers.icc_registers.ICCBoardEEPROM
- SetEEPROM() : optoICC.registers.icc_registers.DeviceEEPROM
- setFEautostart() : optoICC.registers.icc_registers.ICCBoardEEPROM
- SetFeedbackMode() : optoICC.registers.icc_registers.ICCMiscFeatures
- SetFEpower() : optoICC.registers.icc_registers.ICCMiscFeatures
- setFEvoltage() : optoICC.registers.icc_registers.ICCBoardEEPROM
- SetFEvoltage() : optoICC.registers.icc_registers.ICCMiscFeatures
- SetFocalPower() : optoICC.registers.icc_registers.ICCStaticInput
- SetGain() : optoICC.registers.icc_registers.TransformationStage
- SetGain_Variable() : optoICC.registers.icc_registers.LensCompensation
- SetGPIOdirection() : optoICC.registers.icc_registers.ICCMiscFeatures
- SetGPIOstate() : optoICC.registers.icc_registers.ICCMiscFeatures
- setI2Caddr() : optoICC.registers.icc_registers.ICCBoardEEPROM
- setIPv4addr() : optoICC.registers.icc_registers.ICCBoardEEPROM
- setIPv4dns() : optoICC.registers.icc_registers.ICCBoardEEPROM
- setIPv4gateway() : optoICC.registers.icc_registers.ICCBoardEEPROM
- setIPv4subnet() : optoICC.registers.icc_registers.ICCBoardEEPROM
- setIPv6addr() : optoICC.registers.icc_registers.ICCBoardEEPROM
- setIPv6dns() : optoICC.registers.icc_registers.ICCBoardEEPROM
- setIPv6gateway() : optoICC.registers.icc_registers.ICCBoardEEPROM
- setIPv6subnet() : optoICC.registers.icc_registers.ICCBoardEEPROM
- SetLoggedRegister() : optoICC.registers.icc_registers.WindowAverager
- setMACaddr() : optoICC.registers.icc_registers.ICCBoardEEPROM
- SetMatrix() : optoICC.registers.icc_registers.TempCompensation , optoICC.registers.icc_registers.TransformationStage
- SetMatrixAsVector() : optoICC.registers.icc_registers.TempCompensation , optoICC.registers.icc_registers.TransformationStage
- setMaxNegCurrent() : optoICC.registers.icc_registers.DeviceEEPROM
- setMaxPosCurrent() : optoICC.registers.icc_registers.DeviceEEPROM
- SetMode() : optoICC.registers.icc_registers.TempCompensation
- setMode() : optoICC.registers.icc_registers.WaveformAdaptation
- SetOffset() : optoICC.registers.icc_registers.TransformationStage
- setOStempHyst() : optoICC.registers.icc_registers.ICCBoardEEPROM
- setOStempLimit() : optoICC.registers.icc_registers.ICCBoardEEPROM
- SetOutputState() : optoICC.registers.icc_registers.ICCMiscFeatures
- SetPart_config() : optoICC.registers.icc_registers.LensCompensation
- SetPatternSegment() : optoICC.registers.icc_registers.TempCompensation , optoICC.registers.icc_registers.TransformationStage
- setPStempHyst() : optoICC.registers.icc_registers.ICCBoardEEPROM
- setPStempLimit() : optoICC.registers.icc_registers.ICCBoardEEPROM
- setPWMenableChanMask() : optoICC.registers.icc_registers.ICCBoardEEPROM
- setPWMfreq() : optoICC.registers.icc_registers.ICCBoardEEPROM
- SetPWMfrequency() : optoICC.registers.icc_registers.ICCMiscFeatures
- SetSamplingFrequency() : optoICC.registers.icc_registers.WindowAverager
- setSerialNumber() : optoICC.registers.icc_registers.DeviceEEPROM , optoICC.registers.icc_registers.ICCBoardEEPROM
- setSlaveNumOfRegisters() : optoICC.registers.icc_registers.ICCBoardEEPROM
- setTCPIPport() : optoICC.registers.icc_registers.ICCBoardEEPROM
- setUDPport() : optoICC.registers.icc_registers.ICCBoardEEPROM
- SetWcState() : optoICC.registers.icc_registers.ICCMiscFeatures
- sleep() : optoICC.registers.icc_registers.CapacitiveFeedback
- start_accel_readout() : optoICC.registers.icc_registers.InertialMeasurementUnit
- start_controller() : optoICC.registers.icc_registers.SarynControl
- start_gyro_readout() : optoICC.registers.icc_registers.InertialMeasurementUnit
- start_optical_stabilisation() : optoICC.registers.icc_registers.SarynControl
- start_readout() : optoICC.registers.icc_registers.CapacitiveFeedback , optoICC.registers.icc_registers.HallFeedback , optoICC.registers.icc_registers.HallReadout4Lyra
- stop_accel_readout() : optoICC.registers.icc_registers.InertialMeasurementUnit
- stop_controller() : optoICC.registers.icc_registers.SarynControl
- stop_gyro_readout() : optoICC.registers.icc_registers.InertialMeasurementUnit
- stop_optical_stabilisation() : optoICC.registers.icc_registers.SarynControl
- stop_readout() : optoICC.registers.icc_registers.CapacitiveFeedback , optoICC.registers.icc_registers.HallFeedback , optoICC.registers.icc_registers.HallReadout4Lyra
- StopLogger() : optoICC.registers.icc_registers.WindowAverager