| optoICC

Here is a list of all class members with links to the classes they belong to:

### - r -

- rcount_a : optoICC.registers.icc_registers.CapacitiveFeedback
- rcount_b : optoICC.registers.icc_registers.CapacitiveFeedback
- rcount_c : optoICC.registers.icc_registers.CapacitiveFeedback
- register_log_0 : optoICC.registers.icc_registers.WindowAverager
- register_log_1 : optoICC.registers.icc_registers.WindowAverager
- register_log_2 : optoICC.registers.icc_registers.WindowAverager
- register_log_3 : optoICC.registers.icc_registers.WindowAverager
- register_log_4 : optoICC.registers.icc_registers.WindowAverager
- register_log_5 : optoICC.registers.icc_registers.WindowAverager
- reparse : optoICC.registers.icc_registers.DeviceEEPROM
- ReparseEEPROM() : optoICC.registers.icc_registers.DeviceEEPROM
- resdev_a : optoICC.registers.icc_registers.CapacitiveFeedback
- resdev_b : optoICC.registers.icc_registers.CapacitiveFeedback
- resdev_c : optoICC.registers.icc_registers.CapacitiveFeedback
- reset_FW : optoICC.registers.icc_registers.ICCMiscFeatures
- reset_init_done() : optoICC.registers.icc_registers.HallFeedback
- reset_iteration : optoICC.registers.icc_registers.WaveformAdaptation
- reset_stat : optoICC.registers.icc_registers.WindowAverager
- reset_statistics : optoICC.registers.icc_registers.WaveformAdaptation
- reset_values : optoICC.registers.icc_registers.WindowAverager
- ResetAverage() : optoICC.registers.icc_registers.WindowAverager
- ResetAverageContinous() : optoICC.registers.icc_registers.WindowAverager
- ResetAverageKeepFirst() : optoICC.registers.icc_registers.WindowAverager
- ResetCoeffs() : optoICC.registers.icc_registers.LinearizationStage
- ResetFW() : optoICC.registers.icc_registers.ICCMiscFeatures
- ResetStatistics() : optoICC.registers.icc_registers.WindowAverager
- ResetWarningFlagRegister() : optoICC.registers.icc_registers.ICCStatus
- Resolution : optoICC.registers.icc_registers.HallReadout4Lyra
- rms_error : optoICC.registers.icc_registers.WaveformAdaptation
- rms_error_max : optoICC.registers.icc_registers.WaveformAdaptation
- rms_error_z : optoICC.registers.icc_registers.WaveformAdaptation
- rms_spec : optoICC.registers.icc_registers.WaveformAdaptation
- run : optoICC.registers.icc_registers.WaveformAdaptation , optoICC.registers.icc_registers.WindowAverager
- run_controller : optoICC.registers.icc_registers.SarynControl
- run_os : optoICC.registers.icc_registers.SarynControl
- RunInit : optoICC.registers.icc_registers.HallReadout4Lyra
- RunLogger() : optoICC.registers.icc_registers.WindowAverager
- RunReadout : optoICC.registers.icc_registers.HallReadout4Lyra