| optoICC

Loading...
Searching...
No Matches
Here is a list of all class members with links to the classes they belong to:

### - m -

- M : optoICC.registers.icc_registers.TempCompensation, optoICC.registers.icc_registers.TransformationStage
- MAC_addr : optoICC.registers.icc_registers.ICCBoardEEPROM
- map_channels : optoICC.registers.icc_registers.CapacitiveFeedback, optoICC.registers.icc_registers.HallFeedback
- map_channels_hf : optoICC.registers.icc_registers.HallFeedback
- map_channels_temp : optoICC.registers.icc_registers.HallFeedback
- map_channels_temp_gain : optoICC.registers.icc_registers.HallFeedback
- map_channels_temp_offset : optoICC.registers.icc_registers.HallFeedback
- map_channels_temp_raw : optoICC.registers.icc_registers.HallFeedback
- map_channelscf : optoICC.registers.icc_registers.CapacitiveFeedback
- map_channelsref : optoICC.registers.icc_registers.CapacitiveFeedback
- max_gua_temperature : optoICC.registers.icc_registers.LensCompensation
- max_lim_red : optoICC.registers.icc_registers.LensCompensation
- max_lim_scroll : optoICC.registers.icc_registers.LensCompensation
- max_lim_yellow : optoICC.registers.icc_registers.LensCompensation
- max_neg_current : optoICC.registers.icc_registers.DeviceEEPROM
- max_pos_current : optoICC.registers.icc_registers.DeviceEEPROM
- maximum_current : optoICC.registers.icc_registers.ICCAnalogInput
- maximum_dpt : optoICC.registers.icc_registers.ICCAnalogInput
- mcu_id : optoICC.registers.icc_registers.ICCStatus
- mcu_load : optoICC.registers.icc_registers.ICCStatus
- mcu_overload_counter : optoICC.registers.icc_registers.ICCStatus
- mcu_type : optoICC.registers.icc_registers.ICCStatus
- MeasDelay : optoICC.registers.icc_registers.HallReadout4Lyra
- min_gua_temperature : optoICC.registers.icc_registers.LensCompensation
- min_lim_red : optoICC.registers.icc_registers.LensCompensation
- min_lim_scroll : optoICC.registers.icc_registers.LensCompensation
- min_lim_yellow : optoICC.registers.icc_registers.LensCompensation
- minimum_current : optoICC.registers.icc_registers.ICCAnalogInput
- minimum_dpt : optoICC.registers.icc_registers.ICCAnalogInput
- MiscFeatures : optoICC.ecc1c.ECC1cBoard, optoICC.icc4c.ICC4cBoard
- mode : optoICC.registers.icc_registers.TempCompensation, optoICC.registers.icc_registers.WaveformAdaptation
- mu : optoICC.registers.icc_registers.WindowAverager
- muxcfg_a : optoICC.registers.icc_registers.CapacitiveFeedback
- muxcfg_b : optoICC.registers.icc_registers.CapacitiveFeedback
- muxcfg_c : optoICC.registers.icc_registers.CapacitiveFeedback