| optoICC

Loading...
Searching...
No Matches
Public Member Functions | Static Public Member Functions | Public Attributes | Static Protected Attributes | List of all members
optoICC.registers.icc_registers.ICCTemperatureManager Class Reference
Inheritance diagram for optoICC.registers.icc_registers.ICCTemperatureManager:

## Public Member Functions
| __init__ (self, board=None)
| GetDeviceTemperature (self)
| Gets actual device temperature of the active channel.
| GetDeviceTemperatureThreshold (self)
| Gets device temperature threshold of the active channel.
| SetDeviceTemperatureThreshold (self, threshold=0)
| Sets device temperature threshold of the active channel.
| GetBoardOutTemperature (self)
| Gets driver output stage temperature.
| GetBoardOutTemperatureThreshold (self)
| Gets driver output stage temperature threshold.
| SetBoardOutTemperatureThreshold (self, threshold=0)
| Sets driver output stage temperature threshold.
| GetBoardPowTemperature (self)
| Gets driver power supply temperature.
| GetBoardPowTemperatureThreshold (self)
| Gets driver power supply temperature threshold.
| SetBoardPowTemperatureThreshold (self, threshold=0)
| Sets driver power supply temperature threshold.

## Static Public Member Functions
| help ()

## Public Attributes
| sys_id
| device_temperature
| device_temp_threshold
| board_out_temperature
| board_out_threshold
| board_pwr_temperature
| board_pwr_threshold

## Static Protected Attributes
bool | _is_a_system = False

## Detailed Description

    Device Functionality - Device Temperature Readout
    System ID: 0x22

    * | Address | Name                                      | Default | Description     | Type  | Access
    * |---------|-------------------------------------------|---------|-----------------|-------|-----------
    * | 0x2200  | Device temperature                        | N/A     | Degrees Celsius | uint8 | read only
    * | 0x2201  | Device temperature threshold              | 80      | Degrees Celsius. If this threshold is reached the output of the driver is disabled to cool down. Temperature has to fall by 10 degrees so that the output is enabled again | uint8 | read write
    * | 0x2202  | Driver output stage temperature           | N/A     | Degrees Celsius | uint32 | read only
    * | 0x2203  | Driver output stage temperature threshold | 80      | Degrees Celsius. If this threshold is reached the output of the driver is disabled to cool down. Temperature has to fall by 10 degrees so that the output is enabled again | uint32 | read/write
    * | 0x2204  | Driver power supply temperature           | N/A     | Degrees Celsius | uint8 | read only
    * | 0x2205  | Driver power supply temperature threshold | 80      | Degrees Celsius. If this threshold is reached the output of the driver is disabled to cool down. Temperature has to fall by 10 degrees so that the output is enabled again | uint8 | read write

## Constructor & Destructor Documentation

## ◆ __init__()

optoICC.registers.icc_registers.ICCTemperatureManager.__init__ | ( |  | self,
|  |  | board = None )

## Member Function Documentation

## ◆ GetBoardOutTemperature()

optoICC.registers.icc_registers.ICCTemperatureManager.GetBoardOutTemperature | ( |  | self | ) |

Gets driver output stage temperature.

## ◆ GetBoardOutTemperatureThreshold()

optoICC.registers.icc_registers.ICCTemperatureManager.GetBoardOutTemperatureThreshold | ( |  | self | ) |

Gets driver output stage temperature threshold.

If this threshold is reached the output of the driver is disabled to cool down. Temperature has to fall by 10 degrees so that the output is enabled again

## ◆ GetBoardPowTemperature()

optoICC.registers.icc_registers.ICCTemperatureManager.GetBoardPowTemperature | ( |  | self | ) |

Gets driver power supply temperature.

## ◆ GetBoardPowTemperatureThreshold()

optoICC.registers.icc_registers.ICCTemperatureManager.GetBoardPowTemperatureThreshold | ( |  | self | ) |

Gets driver power supply temperature threshold.

If this threshold is reached the output of the driver is disabled to cool down. Temperature has to fall by 10 degrees so that the output is enabled again

## ◆ GetDeviceTemperature()

optoICC.registers.icc_registers.ICCTemperatureManager.GetDeviceTemperature | ( |  | self | ) |

Gets actual device temperature of the active channel.

Active cahnnel is set by 'Status.SetDeviceEEPROMactiveChannel(channel_index)'. This temperature can be also obtained by channel's TemperatureManager 'Channel_0.TemperatureManager.GetDeviceTemperature()'

## ◆ GetDeviceTemperatureThreshold()

optoICC.registers.icc_registers.ICCTemperatureManager.GetDeviceTemperatureThreshold | ( |  | self | ) |

Gets device temperature threshold of the active channel.

Active cahnnel is set by 'Status.SetDeviceEEPROMactiveChannel(channel_index)'. If this threshold is reached the output of the driver is disabled to cool down. Temperature has to fall by 10 degrees so that the output is enabled again. This temperature threshold can be also obtained by channel's TemperatureManager 'Channel_0.TemperatureManager.GetDeviceTemperatureThreshold()'

## ◆ help()

optoICC.registers.icc_registers.ICCTemperatureManager.help | ( |  | ) |
| static

## ◆ SetBoardOutTemperatureThreshold()

optoICC.registers.icc_registers.ICCTemperatureManager.SetBoardOutTemperatureThreshold | ( |  | self,
|  |  | threshold = 0 )

Sets driver output stage temperature threshold.

If this threshold is reached the output of the driver is disabled to cool down. Temperature has to fall by 10 degrees so that the output is enabled again

## ◆ SetBoardPowTemperatureThreshold()

optoICC.registers.icc_registers.ICCTemperatureManager.SetBoardPowTemperatureThreshold | ( |  | self,
|  |  | threshold = 0 )

Sets driver power supply temperature threshold.

If this threshold is reached the output of the driver is disabled to cool down. Temperature has to fall by 10 degrees so that the output is enabled again

## ◆ SetDeviceTemperatureThreshold()

optoICC.registers.icc_registers.ICCTemperatureManager.SetDeviceTemperatureThreshold | ( |  | self,
|  |  | threshold = 0 )

Sets device temperature threshold of the active channel.

Active cahnnel is set by 'Status.SetDeviceEEPROMactiveChannel(channel_index)'. If this threshold is reached the output of the driver is disabled to cool down. Temperature has to fall by 10 degrees so that the output is enabled again. This temperature threshold can be also obtained by channel's TemperatureManager 'Channel_0.TemperatureManager.GetDeviceTemperatureThreshold()'

## Member Data Documentation

## ◆ _is_a_system

bool optoICC.registers.icc_registers.ICCTemperatureManager._is_a_system = False
| static protected

## ◆ board_out_temperature

optoICC.registers.icc_registers.ICCTemperatureManager.board_out_temperature

## ◆ board_out_threshold

optoICC.registers.icc_registers.ICCTemperatureManager.board_out_threshold

## ◆ board_pwr_temperature

optoICC.registers.icc_registers.ICCTemperatureManager.board_pwr_temperature

## ◆ board_pwr_threshold

optoICC.registers.icc_registers.ICCTemperatureManager.board_pwr_threshold

## ◆ device_temp_threshold

optoICC.registers.icc_registers.ICCTemperatureManager.device_temp_threshold

## ◆ device_temperature

optoICC.registers.icc_registers.ICCTemperatureManager.device_temperature

## ◆ sys_id

optoICC.registers.icc_registers.ICCTemperatureManager.sys_id

The documentation for this class was generated from the following file:

- C:/git/145-713-00_optoICC/src/main/python/optoICC/registers/icc_registers.py