| optoMDC

Loading...
Searching...
No Matches
Here is a list of all class members with links to the classes they belong to:

### - g -

- get_fpga_status_register : optoMDC.registers.mre2_registers.MRE2MiscFeatures
- get_natural_freq : optoMDC.registers.mre2_registers.ResonantAmplitudeControl
- get_values() : optoMDC.tools.pyMDC_SPI.SPI
- GetActiveType() : optoMDC.registers.mre3_registers.MRE3StaticInput
- GetActualAmplitude() : optoMDC.registers.mre2_registers.ResonantAmplitudeControl
- GetActualFOV() : optoMDC.registers.mre2_registers.ResonantAmplitudeControl
- GetADCcurrent() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetADCvoltage() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetAnalogInput() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetAngle() : optoMDC.registers.mre2_registers.MRE2StaticInput
- GetAngleA() : optoMDC.registers.mre2_registers.OpticalFeedback
- GetAngleB() : optoMDC.registers.mre2_registers.OpticalFeedback
- GetAverageInputPower() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetAveragingCycles() : optoMDC.registers.mre2_registers.ResonantAmplitudeControl
- GetBoardEppromParsingResults() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetBoardOutTemperature() : optoMDC.registers.mre3_registers.MRE3TemperatureManager
- GetBoardOutTemperatureThreshold() : optoMDC.registers.mre3_registers.MRE3TemperatureManager
- GetBoardPowTemperature() : optoMDC.registers.mre3_registers.MRE3TemperatureManager
- GetBoardPowTemperatureThreshold() : optoMDC.registers.mre3_registers.MRE3TemperatureManager
- GetCalTimestamp() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetControlCycles() : optoMDC.registers.mre2_registers.ResonantAmplitudeControl
- GetControlMode() : optoMDC.mre2.MRE2Channel
- GetControlSetup() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetControlState() : optoMDC.registers.mre2_registers.ResonantAmplitudeControl
- GetCPUFPGAVersion() : optoMDC.registers.mre2_registers.MRE2Status
- GetCurrent() : optoMDC.registers.mre3_registers.MRE3StaticInput
- GetDesiredAmplitude() : optoMDC.registers.mre2_registers.ResonantAmplitudeControl
- GetDesiredFOV() : optoMDC.registers.mre2_registers.ResonantAmplitudeControl
- GetDevice3V3chanMask() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetDeviceDetectChanMask() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetDeviceDetectSwitchMask() : optoMDC.registers.mre3_registers.MRE3Status
- GetDeviceEEPROMactiveChannel() : optoMDC.registers.mre3_registers.MRE3Status
- GetDevicePower() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetDevicePowerMask() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetDeviceStatus() : optoMDC.registers.mre3_registers.MRE3Status
- GetDeviceTemperature() : optoMDC.registers.mre3_registers.MRE3TemperatureManager
- GetDeviceTemperatureThreshold() : optoMDC.registers.mre3_registers.MRE3TemperatureManager
- GetDeviceType() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetDriveCurrent() : optoMDC.registers.mre2_registers.ResonantAmplitudeControl
- GetDriveFreq() : optoMDC.registers.mre2_registers.ResonantAmplitudeControl
- GetEepromSubVersion() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetEepromVersion() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetFEautostart() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetFeedbackMode() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetFEpower() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetFEvoltage() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM, optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetFilteredPDValues() : optoMDC.registers.mre2_registers.OpticalFeedback
- GetFPGAStatusRegister() : optoMDC.registers.mre2_registers.MRE2MiscFeatures
- GetFreqDelta() : optoMDC.registers.mre2_registers.ResonantAmplitudeControl
- GetFreqShift() : optoMDC.registers.mre2_registers.ResonantAmplitudeControl
- GetFreqTolerance() : optoMDC.registers.mre2_registers.ResonantAmplitudeControl
- GetGPIOdirection() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetGPIOstate() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetI2Caddr() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetI2CList() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetIIN() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetLog() : optoMDC.registers.mre3_registers.Logger
- GetLoggedRegister() : optoMDC.registers.mre3_registers.Logger
- GetMCUid() : optoMDC.registers.mre3_registers.MRE3Status
- GetMCUload() : optoMDC.registers.mre3_registers.MRE3Status
- GetMCUoverloadCounter() : optoMDC.registers.mre3_registers.MRE3Status
- GetMcuTemperature() : optoMDC.registers.mre3_registers.MRE3TemperatureManager
- GetMcuTemperatureThreshold() : optoMDC.registers.mre3_registers.MRE3TemperatureManager
- GetMCUtype() : optoMDC.registers.mre3_registers.MRE3Status
- GetMirrorCoordinateX() : optoMDC.registers.mre3_registers.RadialBasisFunction
- GetMirrorCoordinateY() : optoMDC.registers.mre3_registers.RadialBasisFunction
- GetNaturalFreq() : optoMDC.registers.mre2_registers.ResonantAmplitudeControl
- GetNegativeCurrentLimitChannel0() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetNegativeCurrentLimitChannel1() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetOF() : optoMDC.registers.mre2_registers.MRE2StaticInput, optoMDC.registers.mre3_registers.MRE3StaticInput
- GetOperationMode() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetOpticalFeedbackA() : optoMDC.registers.mre2_registers.OpticalFeedback, optoMDC.registers.mre3_registers.OpticalFeedback
- GetOpticalFeedbackB() : optoMDC.registers.mre2_registers.OpticalFeedback, optoMDC.registers.mre3_registers.OpticalFeedback
- GetOStempHyst() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetOStempLimit() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetOutputState() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetPDValues() : optoMDC.registers.mre2_registers.OpticalFeedback
- GetPositionX() : optoMDC.registers.mre2_registers.OpticalFeedback
- GetPositionY() : optoMDC.registers.mre2_registers.OpticalFeedback
- GetPositiveCurrentLimitChannel0() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetPositiveCurrentLimitChannel1() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetPowerOnDelay() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetProxyFPGAVersion() : optoMDC.registers.mre2_registers.MRE2Status
- GetProxyTemperature() : optoMDC.registers.mre2_registers.MRE2TemperatureManager
- GetProxyTemperatureThreshold() : optoMDC.registers.mre2_registers.MRE2TemperatureManager
- GetPStempHyst() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetPStempLimit() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetPWMenableChanMask() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetPWMfreq() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetPWMfrequency() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetResistance() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetResonanceSlope() : optoMDC.registers.mre2_registers.ResonantAmplitudeControl
- GetSamplingFrequency() : optoMDC.registers.mre3_registers.Logger
- GetScutiLED() : optoMDC.registers.mre2_registers.MRE2MiscFeatures
- GetScutiTemperature() : optoMDC.registers.mre2_registers.MRE2TemperatureManager
- GetScutiTemperatureThreshold() : optoMDC.registers.mre2_registers.MRE2TemperatureManager
- GetSerialNumber() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetSlaveNumOfRegisters() : optoMDC.registers.mre3_registers.MRE3BoardEEPROM
- GetTimeWindow() : optoMDC.registers.mre2_registers.ResonantAmplitudeControl
- GetUFE() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetUIN() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetWcState() : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GetXY() : optoMDC.registers.mre2_registers.MRE2StaticInput, optoMDC.registers.mre3_registers.MRE3StaticInput
- GPIO_DIRECTION : optoMDC.registers.mre3_registers.MRE3MiscFeatures
- GPIO_STATE : optoMDC.registers.mre3_registers.MRE3MiscFeatures