optoKummenberg

Loading...
Searching...
No Matches
optoKummenberg.registers.MiscSystems.Manager Class Reference
Inheritance diagram for optoKummenberg.registers.MiscSystems.Manager:

## Public Member Functions
| __init__ (self, int channel=0, board=None)
| CheckSignalFlow (self)
Public Member Functions inherited from optoKummenberg.registers.ClassAbstracts.System
| __init__ (self, int or None channel=None, board=None)
| set_register (self, str or int register_name_or_id, value, bool set_internal=False)
| set_register_id (self, int register_id, value, type=None)
| get_register (self, str or int register_name_or_id)
| get_register_id (self, int register_id)
| get_register_names (self)

## Static Public Member Functions
| help ()

## Public Attributes
int | sys_id = 0x40
dict | input
dict | input_conditioning
dict | control
dict | output_conditioning
dict | output
Public Attributes inherited from optoKummenberg.registers.ClassAbstracts.System
| name = self.__class__.__name__
| register_list = self._get_register_list()

## Protected Attributes
bool | _readonly = False
Protected Attributes inherited from optoKummenberg.registers.ClassAbstracts.System
| _channel = channel
| _board = board

## Additional Inherited Members
Protected Member Functions inherited from optoKummenberg.registers.ClassAbstracts.System
| _get_register_list (self)
Static Protected Attributes inherited from optoKummenberg.registers.ClassAbstracts.System
bool | _is_a_system = False

## Detailed Description

    The Signal Flow Channel Manager is managing the active systems in the signal flow chain.
    System ID for channel X: 0x40

    +---------------------+---------------+-------------+----------+--------------+---------------+--------------------+
    | Register Name       | Id            | Type        | Unit     | Range        | Default       | Comment            |
    +=====================+===============+=============+==========+==============+===============+====================+
    | input               | 5xCHANNEL + 0 | uint 32-bit | SystemID | 0x48 to 0x7f |               |                    |
    +---------------------+---------------+-------------+----------+--------------+---------------+--------------------+
    | input_conditioning  | 5xCHANNEL + 1 | uint 32-bit | SystemID | 0x48 to 0x7f |               |                    |
    +---------------------+---------------+-------------+----------+--------------+---------------+--------------------+
    | control             | 5xCHANNEL + 2 | uint 32-bit | SystemID | 0x48 to 0x7f |               |                    |
    +---------------------+---------------+-------------+----------+--------------+---------------+--------------------+
    | output_conditioning | 5xCHANNEL + 3 | uint 32-bit | SystemID | 0x48 to 0x7f |               |                    |
    +---------------------+---------------+-------------+----------+--------------+---------------+--------------------+
    | output              | 5*CHANNEL + 4 | uint 32-bit | SystemID | 0x48 to 0x7f |               |                    |
    +---------------------+---------------+-------------+----------+--------------+---------------+--------------------+

## Constructor & Destructor Documentation

## ◆ __init__()

optoKummenberg.registers.MiscSystems.Manager.__init__ | ( |  | self,
|  | int | channel = 0,
|  |  | board = None )

## Member Function Documentation

## ◆ CheckSignalFlow()

optoKummenberg.registers.MiscSystems.Manager.CheckSignalFlow | ( |  | self | ) |

## ◆ help()

optoKummenberg.registers.MiscSystems.Manager.help | ( |  | ) |
| static

## Member Data Documentation

## ◆ _readonly

bool optoKummenberg.registers.MiscSystems.Manager._readonly = False
| protected

## ◆ control

dict optoKummenberg.registers.MiscSystems.Manager.control

Initial value:
= {'name': 'control',
'id': self.sys_id << 8 | channel * 5 + 0x02,
'type': int,
'unit': None,
'range': None,
'default': None,
'value': None}

## ◆ input

dict optoKummenberg.registers.MiscSystems.Manager.input

Initial value:
= {'id': self.sys_id << 8 | channel * 5 + 0x00,
'type': int,
'unit': 'SystemID',
'range': [0x48, 0x7f],
'default': None,
'value': None}

## ◆ input_conditioning

dict optoKummenberg.registers.MiscSystems.Manager.input_conditioning

Initial value:
= {'name': 'input_conditioning',
'id': self.sys_id << 8 | channel * 5 + 0x01,
'type': int,
'unit': 'SystemID',
'range': [0x48, 0x7f],
'default': None,
'value': None}

## ◆ output

dict optoKummenberg.registers.MiscSystems.Manager.output

Initial value:
= {'name': 'output',
'id': self.sys_id << 8 | channel * 5 + 0x04,
'type': int,
'unit': 'SystemID',
'range': [0x48, 0xef],
'default': None,
'value': None}

## ◆ output_conditioning

dict optoKummenberg.registers.MiscSystems.Manager.output_conditioning

Initial value:
= {'name': 'output_conditioning',
'id': self.sys_id << 8 | channel * 5 + 0x03,
'type': int,
'unit': 'SystemID',
'range': [0x48, 0x7f],
'default': None,
'value': None}

## ◆ sys_id

int optoKummenberg.registers.MiscSystems.Manager.sys_id = 0x40

The documentation for this class was generated from the following file:

- C:/git/142-421-00_optoKummenberg/src/main/python/optoKummenberg/registers/MiscSystems.py