MR-E-2 SDK

MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController Member List

This is the complete list of members for MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController, including all inherited members.

AssignProducts() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ChangeActiveControlModeStageSystem(EMrE2ControlModeSystems mrE2ControlModeSystem, EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ChangeActiveInputStageSystem(EAxis axis, EmrE2InputStageSystems inputStageSystem) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ChangeModeToPro() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ChangeModeToSimple() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
CleanUpDevice() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
Connect(IIpAddressPortPair ipPair) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
Connect(IDevicePort port) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
Disconnect() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ElectronicsType (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController |
GetBoardEepromBytes(int index, int length) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetBoardFirmwareBranch() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetBoardFirmwareBuildVersion() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetBoardFirmwareId() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetBoardFirmwareMajorVersion() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetBoardFirmwareMinorVersion() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetBoardFirmwareRevisionVersion() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetBoardFirmwareType() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetCpuFpgaVersion() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetDeviceStatus() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetEepromSubVersion() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetEepromVersion() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetElectronicProperties() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetElectronicSerialNumber() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetFirmwareSerialNumber() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetGitHeadSha1() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetMaxNegativeCurrent() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetMaxPositiveCurrent() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetMirrorEepromBytes(int index, int length) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetPartConfiguration() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetPartConfigurationVersion() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetProductProperties(ProductProperties productProperty) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetProductSerialNumber() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetProxyFpgaVersion() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetTemperatureGradientA() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetTemperatureGradientB() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetTemperatureOffsetA() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GetTemperatureOffsetB() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
GoToDfuMode() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
IsConnected() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
IsLoggerRunning() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
LoadSnapshot(int snapshotNumber) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
LockBoardEepromWriting() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
LockMirrorEepromWriting() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
MiscellaneousFeaturesDumpBoardEepromMappedMemory() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
MiscellaneousFeaturesDumpDeviceEepromMappedMemory() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
MiscellaneousFeaturesDumpFpgaMappedMemory() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
MiscellaneousFeaturesResetFirmware() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
MiscellaneousFeaturesSwitchCpuBoardStatusLed(bool enabled) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
MiscellaneousFeaturesSwitchProxyBoardStatusLed(bool enabled) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
MiscellaneousFeaturesSwitchProxyFpgaClock(bool enabled) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
MrE2ForMr15Dash30DeviceController(ElectronicProperties electronicProperties) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ProductTypesList (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController |
ReadActiveControlModeStageSystem(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadActiveInputStageSystem(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadArbitraryVectorValues(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidCutOffFrequency(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidDerivativeGainConstantTerm(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidDerivativeGainLinearTermMultiplier(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidDerivativeGainQuadraticTermMultiplier(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidDerivativeTermFilterEnabled(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidDesiredSetPoint(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidDGain(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidGainScheduling(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidGainSchedulingVariable(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidIGain(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidIntegralGainConstantTerm(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidIntegralGainLinearTermMultiplier(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidIntegralGainQuadraticTermMultiplier(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidMaximumIntegral(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidMaximumOutput(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidMinimumIntegral(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidMinimumOutput(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidPGain(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidProportionalGainConstantTerm(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidProportionalGainLinearTermMultiplier(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeAnglePidProportionalGainQuadraticTermMultiplier(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidCutOffFrequency(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidDerivativeGainConstantTerm(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidDerivativeGainLinearTermMultiplier(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidDerivativeGainQuadraticTermMultiplier(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidDerivativeTermFilterEnabled(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidDesiredSetPoint(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidDGain(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidGainScheduling(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidGainSchedulingVariable(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidIGain(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidIntegralGainConstantTerm(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidIntegralGainLinearTermMultiplier(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidIntegralGainQuadraticTermMultiplier(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidMaximumIntegral(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidMaximumOutput(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidMinimumIntegral(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidMinimumOutput(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidPGain(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidProportionalGainConstantTerm(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidProportionalGainLinearTermMultiplier(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadControlModeOfPidProportionalGainQuadraticTermMultiplier(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadI2CReadPointer0Address() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadI2CReadPointer1Address() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputConditioningOffsetAndScaleOffset(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputConditioningOffsetAndScaleScale(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalActiveStaticInputType(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalAnalogInputActiveInputType(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalAnalogInputAdcRawValue(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalAnalogInputCycles(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalAnalogInputExternalTrigger(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalAngle(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalArbitraryVectorMaximumSamplingRate(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalArbitraryVectorMinimumSamplingRate(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalArbitraryVectorRunning(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalArbitraryVectorSampleRate(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalArbitraryVectorUnit(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalCurrent(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalOpticalFeedback(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalSignalGenerator(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalSignalGeneratorAmplitude(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalSignalGeneratorCycles(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalSignalGeneratorDutyCycles(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalSignalGeneratorExternalTrigger(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalSignalGeneratorFrequency(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalSignalGeneratorOffset(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalSignalGeneratorPhaseDelay(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalSignalGeneratorRunning(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalSignalGeneratorShape(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadInputSignalSignalGeneratorUnit(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadLinearOutputStageActualCurrent(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadLinearOutputStageAverageLimitPeriod(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadLinearOutputStageAverageLimitSum(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadLinearOutputStageChannelNumber(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadLinearOutputStageCooldownPeriod(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadLinearOutputStageCurrentLimit(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadLoggedRegisterAddress(int registerNumber) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadLoggerMaximumSamplingFrequency() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadLoggerMinimumSamplingFrequency() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadLoggerRegisterLog(int registerNumber, int startIndex=0, int endIndex=5000) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadLoggerSamplingRate() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadMiscellaneousFeaturesBoardEepromDumpSize() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadMiscellaneousFeaturesDeviceEepromDumpSize() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadMiscellaneousFeaturesFpgaStatusRegister() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadMiscellaneousFeaturesMirrorLedIntensity() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadNumberOfAvailableSnapshots() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadOfManagerActualOutputAngle(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadOfManagerActualOutputOpticalFeedback(EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadOfManagerFilteredPhotoDiodePd0() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadOfManagerFilteredPhotoDiodePd1() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadOfManagerFilteredPhotoDiodePd2() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadOfManagerFilteredPhotoDiodePd3() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadOfManagerRawPhotoDiodePd0() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadOfManagerRawPhotoDiodePd1() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadOfManagerRawPhotoDiodePd2() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadOfManagerRawPhotoDiodePd3() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadOfManagerStabilityCriterionPositionParameterA() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadOfManagerStabilityCriterionPositionParameterB() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadOfManagerStabilityCriterionVelocityParameterA() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadOfManagerStabilityCriterionVelocityParameterB() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadSnapshotManagerErrorRegisterId() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadSnapshotManagerErrorSystemId() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadSnapshotManagerErrorValue() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadSpiReadPointer0Address() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadSpiReadPointer1Address() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadSpiSystemTick() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadStartupSnapshotNumber() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadTemperatureDevice() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadTemperatureDeviceThreshold() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadTemperatureElectronic() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadTemperatureElectronicThreshold() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadVectorAdapterDataSize() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadVectorAdapterErrorFlag() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadVectorAdapterVectorAddress() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadVectorAdapterVectorData() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReadVectorAdapterVectorIndex() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReaI2CErrorResponse0() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReaI2CErrorResponse1() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
Reconnect() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ReparseMirrorEeprom() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
ResetErrorFlags() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
SaveMemoryPersistence() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
SaveSnapshot(int snapshotNumber) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
SetBoardEepromBytes(int index, byte[] bytes) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
SetMirrorEepromBytes(int index, byte[] bytes) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
StartLogger() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
StopLogger() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
SwitchControlModeAnglePidDerivativeTermFilter(EAxis axis, bool enabled) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
SwitchControlModeAnglePidGainScheduling(EAxis axis, bool enabled) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
SwitchControlModeOfPidDerivativeTermFilter(EAxis axis, bool enabled) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
SwitchControlModeOfPidGainScheduling(EAxis axis, bool enabled) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
UnlockBoardEepromWriting() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
UnlockMirrorEepromWriting() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
VectorAdapterReadVector() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
VectorAdapterWriteVector() (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteArbitraryVectorValues(EAxis axis, IList< float > values, int startIndex) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidCutOffFrequency(EAxis axis, float frequency) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidDerivativeGainConstantTerm(EAxis axis, float cD) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidDerivativeGainLinearTermMultiplier(EAxis axis, float bD) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidDerivativeGainQuadraticTermMultiplier(EAxis axis, float aD) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidDGain(EAxis axis, float dGain) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidGainSchedulingVariable(EAxis axis, GainSchedulingVariable variable) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidIGain(EAxis axis, float iGain) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidIntegralGainConstantTerm(EAxis axis, float cI) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidIntegralGainLinearTermMultiplier(EAxis axis, float bI) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidIntegralGainQuadraticTermMultiplier(EAxis axis, float aI) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidMaximumIntegral(EAxis axis, float maximumIntegral) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidMaximumOutput(EAxis axis, float maximumOutput) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidMinimumIntegral(EAxis axis, float minimumIntegral) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidMinimumOutput(EAxis axis, float minimumOutput) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidPGain(EAxis axis, float pGain) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidProportionalGainConstantTerm(EAxis axis, float cP) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidProportionalGainLinearTermMultiplier(EAxis axis, float bP) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeAnglePidProportionalGainQuadraticTermMultiplier(EAxis axis, float aP) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidCutOffFrequency(EAxis axis, float frequency) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidDerivativeGainConstantTerm(EAxis axis, float cD) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidDerivativeGainLinearTermMultiplier(EAxis axis, float bD) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidDerivativeGainQuadraticTermMultiplier(EAxis axis, float aD) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidDGain(EAxis axis, float dGain) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidGainSchedulingVariable(EAxis axis, GainSchedulingVariable variable) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidIGain(EAxis axis, float iGain) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidIntegralGainConstantTerm(EAxis axis, float cI) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidIntegralGainLinearTermMultiplier(EAxis axis, float bI) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidIntegralGainQuadraticTermMultiplier(EAxis axis, float aI) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidMaximumIntegral(EAxis axis, float maximumIntegral) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidMaximumOutput(EAxis axis, float maximumOutput) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidMinimumIntegral(EAxis axis, float minimumIntegral) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidMinimumOutput(EAxis axis, float minimumOutput) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidPGain(EAxis axis, float pGain) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidProportionalGainConstantTerm(EAxis axis, float cP) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidProportionalGainLinearTermMultiplier(EAxis axis, float bP) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteControlModeOfPidProportionalGainQuadraticTermMultiplier(EAxis axis, float aP) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteI2CReadPointer0Address(int address) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteI2CReadPointer1Address(int address) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputConditioningOffsetAndScaleOffset(EAxis axis, float offset) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputConditioningOffsetAndScaleScale(EAxis axis, float scale) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalAnalogInputCycles(EAxis axis, int cycles) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalAnalogInputExternalTrigger(EAxis axis, bool trigger) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalAngle(EAxis axis, float value) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalArbitraryVectorRunning(EAxis axis, bool running) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalArbitraryVectorSampleRate(EAxis axis, float value) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalArbitraryVectorUnit(EAxis axis, EUnitType selectedOption) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalCurrent(EAxis axis, float value) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalOpticalFeedback(EAxis axis, float value) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalSignalGenerator(SignalGeneratorValuesDto singleAxis, EAxis axis) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalSignalGeneratorAmplitude(EAxis axis, float value) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalSignalGeneratorCycles(EAxis axis, int cycles) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalSignalGeneratorDutyCycles(EAxis axis, float dutyCycles) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalSignalGeneratorExternalTrigger(EAxis axis, bool trigger) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalSignalGeneratorFrequency(EAxis axis, float value) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalSignalGeneratorOffset(EAxis axis, float offset) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalSignalGeneratorPhaseDelay(EAxis axis, float phaseDelay) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalSignalGeneratorRunning(EAxis axis, bool isRunning) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalSignalGeneratorShape(EAxis axis, EWaveformShape shape) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteInputSignalSignalGeneratorUnit(EAxis axis, EUnitType unit) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteLinearOutputStageAverageLimitPeriod(EAxis axis, float value) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteLinearOutputStageAverageLimitSum(EAxis axis, float value) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteLinearOutputStageCooldownPeriod(EAxis axis, float value) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteLinearOutputStageCurrentLimit(EAxis axis, float value) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteLoggedRegisterAddress(int registerNumber, ushort registerAddress) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteLoggerSamplingRate(float samplingRate) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteMiscellaneousFeaturesBoardEepromDumpSize(int eepromDumpSize) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteMiscellaneousFeaturesDeviceEepromDumpSize(int eepromDumpSize) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteMiscellaneousFeaturesMirrorLedIntensity(float ledIntensity) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteSpiReadPointer0Address(int address) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteSpiReadPointer1Address(int address) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteStartupSnapshotNumber(int snapshotNumber) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteTemperatureDeviceThreshold(int temperatureThreshold) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteTemperatureElectronicThreshold(int temperatureThreshold) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteVectorAdapterDataSize(uint dataSize) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteVectorAdapterVectorData(byte[] vectorData) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteVectorAdapterVectorIndex(uint vectorIndex) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline
WriteVectorAddress(int vectorAddress) (defined in MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController) | MrE2ModuleSdk.Device.MrE2ForMr15Dash30DeviceController | inline