MR-E-2 SDK

Here is a list of all documented class members with links to the class documentation for each member:

### - g -

- GetBoardFirmwareBranch() : MrE2ModuleSdk.Device.IStatus , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetBoardFirmwareBuildVersion() : MrE2ModuleSdk.Device.IStatus , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetBoardFirmwareId() : MrE2ModuleSdk.Device.IStatus , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetBoardFirmwareMajorVersion() : MrE2ModuleSdk.Device.IStatus , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetBoardFirmwareMinorVersion() : MrE2ModuleSdk.Device.IStatus , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetBoardFirmwareRevisionVersion() : MrE2ModuleSdk.Device.IStatus , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetBoardFirmwareType() : MrE2ModuleSdk.Device.IStatus , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetBytes() : MrE2ModuleSdk.Device.IBoardEeprom , MrE2ModuleSdk.Device.IDeviceEeprom , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetCpuFpgaVersion() : MrE2ModuleSdk.Device.IStatus , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetDeviceStatus() : MrE2ModuleSdk.Device.IStatus , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetEepromSubVersion() : MrE2ModuleSdk.Device.IDeviceEeprom , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetEepromVersion() : MrE2ModuleSdk.Device.IDeviceEeprom , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetElectronicSerialNumber() : MrE2ModuleSdk.Device.IMrE2ForMr15Dash30SdkComDeviceController , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetFirmwareSerialNumber() : MrE2ModuleSdk.Device.IStatus , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetGitHeadSha1() : MrE2ModuleSdk.Device.IStatus , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetMaxNegativeCurrent() : MrE2ModuleSdk.Device.IDeviceEeprom , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetMaxPositiveCurrent() : MrE2ModuleSdk.Device.IDeviceEeprom , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetPartConfiguration() : MrE2ModuleSdk.Device.IDeviceEeprom , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetPartConfigurationVersion() : MrE2ModuleSdk.Device.IDeviceEeprom , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetProductSerialNumber() : MrE2ModuleSdk.Device.IMrE2ForMr15Dash30SdkComDeviceController , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetProxyFpgaVersion() : MrE2ModuleSdk.Device.IStatus , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetTemperatureGradientA() : MrE2ModuleSdk.Device.IDeviceEeprom , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetTemperatureGradientB() : MrE2ModuleSdk.Device.IDeviceEeprom , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetTemperatureOffsetA() : MrE2ModuleSdk.Device.IDeviceEeprom , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GetTemperatureOffsetB() : MrE2ModuleSdk.Device.IDeviceEeprom , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- GoToDfuMode() : MrE2ModuleSdk.Device.IMrE2ForMr15Dash30SdkComDeviceController , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController