\doxysection{Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+IControl\+Mode\+Stage Interface Reference}
\hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage}{}\label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage}\index{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage}}
Inheritance diagram for Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+IControl\+Mode\+Stage\+:\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[height=2.000000cm]{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage}
\end{center}
\end{figure}
\doxysubsubsection*{Public Member Functions}
\begin{DoxyCompactItemize}
\item 
EMr\+EControl\+Mode\+Systems \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage_a51d4020962d8df28a42c039a1fd27cdb}{Read\+Active\+System}} (EAxis axis)
\begin{DoxyCompactList}\small\item\em Returns active control mode system of the axis. \end{DoxyCompactList}\item 
void \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage_a26cb23980a66ad40a95a16d06f22fb18}{Change\+Active\+System}} (EMr\+EControl\+Mode\+Systems mr\+E2\+Control\+Mode\+System, EAxis axis)
\begin{DoxyCompactList}\small\item\em Sets active control mode system of the axis. \end{DoxyCompactList}\item 
void \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage_a2522ef3a9ac4ea5f3e5cdcaeaacc7eb5}{Set\+Operation\+Mode}} (EOperation\+Mode operation\+Mode)
\begin{DoxyCompactList}\small\item\em Set current operation mode in control stage for both axis. \end{DoxyCompactList}\item 
EOperation\+Mode \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage_a5801ad29652141b4b4540d2aebf45771}{Get\+Operation\+Mode}} ()
\begin{DoxyCompactList}\small\item\em Get current operation mode in control stage for both axis. \end{DoxyCompactList}\end{DoxyCompactItemize}
\doxysubsubsection*{Properties}
\begin{DoxyCompactItemize}
\item 
\mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_control_mode_1_1_i_x_y_pid}{IXYPid}} \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage_a17fcadbb98f559b8807f709f37df5ab0}{XYPid}}\hspace{0.3cm}{\ttfamily  \mbox{[}get\mbox{]}}
\end{DoxyCompactItemize}


\doxysubsection{Member Function Documentation}
\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage_a26cb23980a66ad40a95a16d06f22fb18}\index{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage}!ChangeActiveSystem@{ChangeActiveSystem}}
\index{ChangeActiveSystem@{ChangeActiveSystem}!MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage}}
\doxysubsubsection{\texorpdfstring{ChangeActiveSystem()}{ChangeActiveSystem()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage_a26cb23980a66ad40a95a16d06f22fb18} 
void Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+IControl\+Mode\+Stage.\+Change\+Active\+System (\begin{DoxyParamCaption}\item[{EMr\+EControl\+Mode\+Systems}]{mr\+E2\+Control\+Mode\+System}{, }\item[{EAxis}]{axis}{}\end{DoxyParamCaption})}



Sets active control mode system of the axis. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_a563500c2f7f6f800e514b264870a04b2}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage_a5801ad29652141b4b4540d2aebf45771}\index{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage}!GetOperationMode@{GetOperationMode}}
\index{GetOperationMode@{GetOperationMode}!MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage}}
\doxysubsubsection{\texorpdfstring{GetOperationMode()}{GetOperationMode()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage_a5801ad29652141b4b4540d2aebf45771} 
EOperation\+Mode Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+IControl\+Mode\+Stage.\+Get\+Operation\+Mode (\begin{DoxyParamCaption}{}{}\end{DoxyParamCaption})}



Get current operation mode in control stage for both axis. 

\begin{DoxyReturn}{Returns}
Operation\+Mode
\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_a582522c93c1d51c6f52af0f3abd04cbb}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage_a51d4020962d8df28a42c039a1fd27cdb}\index{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage}!ReadActiveSystem@{ReadActiveSystem}}
\index{ReadActiveSystem@{ReadActiveSystem}!MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage}}
\doxysubsubsection{\texorpdfstring{ReadActiveSystem()}{ReadActiveSystem()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage_a51d4020962d8df28a42c039a1fd27cdb} 
EMr\+EControl\+Mode\+Systems Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+IControl\+Mode\+Stage.\+Read\+Active\+System (\begin{DoxyParamCaption}\item[{EAxis}]{axis}{}\end{DoxyParamCaption})}



Returns active control mode system of the axis. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_aed781a0874dd1c84317c3f1f119fb998}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage_a2522ef3a9ac4ea5f3e5cdcaeaacc7eb5}\index{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage}!SetOperationMode@{SetOperationMode}}
\index{SetOperationMode@{SetOperationMode}!MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage}}
\doxysubsubsection{\texorpdfstring{SetOperationMode()}{SetOperationMode()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage_a2522ef3a9ac4ea5f3e5cdcaeaacc7eb5} 
void Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+IControl\+Mode\+Stage.\+Set\+Operation\+Mode (\begin{DoxyParamCaption}\item[{EOperation\+Mode}]{operation\+Mode}{}\end{DoxyParamCaption})}



Set current operation mode in control stage for both axis. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_ac4635df9e20891c15f3c194e3de01944}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.



\doxysubsection{Property Documentation}
\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage_a17fcadbb98f559b8807f709f37df5ab0}\index{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage}!XYPid@{XYPid}}
\index{XYPid@{XYPid}!MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.IControlModeStage}}
\doxysubsubsection{\texorpdfstring{XYPid}{XYPid}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_i_control_mode_stage_a17fcadbb98f559b8807f709f37df5ab0} 
\mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_control_mode_1_1_i_x_y_pid}{IXYPid}} Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+IControl\+Mode\+Stage.\+XYPid\hspace{0.3cm}{\ttfamily [get]}}



Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_a9380184ce00242912cdc6e751df29a3e}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.



The documentation for this interface was generated from the following file\+:\begin{DoxyCompactItemize}
\item 
C\+:/\+Users/jan.\+janda/\+Desktop/\+Mre3\+Documentation/\+Signal\+Flow\+Manager/\mbox{\hyperlink{_i_control_mode_stage_8cs}{IControl\+Mode\+Stage.\+cs}}\end{DoxyCompactItemize}
