MR-E-2 SDK

MrE2ModuleSdk.Device.IOpticalFeedbackPid Member List

This is the complete list of members for MrE2ModuleSdk.Device.IOpticalFeedbackPid, including all inherited members.

IsGainScheduling(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadCutOffFrequency(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadDerivativeGainConstantTerm(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadDerivativeGainLinearTermMultiplier(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadDerivativeGainQuadraticTermMultiplier(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadDerivativeTermFilterEnabled(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadDesiredSetPoint(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadDGain(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadGainSchedulingVariable(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadIGain(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadIntegralGainConstantTerm(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadIntegralGainLinearTermMultiplier(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadIntegralGainQuadraticTermMultiplier(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadMaximumIntegral(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadMaximumOutput(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadMinimumIntegral(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadMinimumOutput(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadPGain(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadProportionalGainConstantTerm(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadProportionalGainLinearTermMultiplier(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
ReadProportionalGainQuadraticTermMultiplier(EAxis axis) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
SwitchDerivativeTermFilter(EAxis axis, bool enabled) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
SwitchGainScheduling(EAxis axis, bool enabled) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WriteCutOffFrequency(EAxis axis, float frequency) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WriteDerivativeGainConstantTerm(EAxis axis, float cD) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WriteDerivativeGainLinearTermMultiplier(EAxis axis, float bD) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WriteDerivativeGainQuadraticTermMultiplier(EAxis axis, float aD) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WriteDGain(EAxis axis, float dGain) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WriteGainSchedulingVariable(EAxis axis, GainSchedulingVariable variable) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WriteIGain(EAxis axis, float iGain) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WriteIntegralGainConstantTerm(EAxis axis, float cI) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WriteIntegralGainLinearTermMultiplier(EAxis axis, float bI) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WriteIntegralGainQuadraticTermMultiplier(EAxis axis, float aI) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WriteMaximumIntegral(EAxis axis, float maximumIntegral) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WriteMaximumOutput(EAxis axis, float maximumOutput) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WriteMinimumIntegral(EAxis axis, float minimumIntegral) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WriteMinimumOutput(EAxis axis, float minimumOutput) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WritePGain(EAxis axis, float pGain) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WriteProportionalGainConstantTerm(EAxis axis, float cP) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WriteProportionalGainLinearTermMultiplier(EAxis axis, float bP) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |
WriteProportionalGainQuadraticTermMultiplier(EAxis axis, float aP) | MrE2ModuleSdk.Device.IOpticalFeedbackPid |