MRE3 C# SDK

Loading...
Searching...
No Matches
Public Member Functions | List of all members
MrEModuleSdk.Devices.SdkInterfaces.IDeviceEEPROM Interface Reference
Inheritance diagram for MrEModuleSdk.Devices.SdkInterfaces.IDeviceEEPROM:

## Public Member Functions
void | SetBytes (int index, byte[] inputBytes)
| Sets EEPROM bytes of the product.
byte[] | GetBytes (int index, int length)
| Returns EEPROM bytes of the product.
int | GetEepromVersion ()
| Returns EEPROM version.
int | GetEepromSubVersion ()
| Returns EEPROM subversion.
int | GetPartConfiguration ()
| Returns part configuration value.
int | GetPartConfigurationVersion ()
| Returns part configuration version value.
int | GetMaxPositiveCurrent ()
| Returns max positive current.
int | GetMaxNegativeCurrent ()
| Returns max negative current.
void | LockMirrorEepromWriting ()
| Locks mirror EEPROM writing.
void | UnlockMirrorEepromWriting ()
| Unlocks mirror EEPROM writing.
void | ReparseMirrorEeprom ()
| Reparse mirror EEPROM.

## Member Function Documentation

## ◆ GetBytes()

byte[] MrEModuleSdk.Devices.SdkInterfaces.IDeviceEEPROM.GetBytes | ( | int | index,
|  | int | length )

Returns EEPROM bytes of the product.

Parameters

  index | Index of the start
  length | Amount of read bytes

Returns

Implemented in MrEModuleSdk.Devices.Mre3.MrE3SdkComDeviceController.

## ◆ GetEepromSubVersion()

int MrEModuleSdk.Devices.SdkInterfaces.IDeviceEEPROM.GetEepromSubVersion | ( |  | ) |

Returns EEPROM subversion.

Returns

Implemented in MrEModuleSdk.Devices.Mre3.MrE3SdkComDeviceController.

## ◆ GetEepromVersion()

int MrEModuleSdk.Devices.SdkInterfaces.IDeviceEEPROM.GetEepromVersion | ( |  | ) |

Returns EEPROM version.

Returns

Implemented in MrEModuleSdk.Devices.Mre3.MrE3SdkComDeviceController.

## ◆ GetMaxNegativeCurrent()

int MrEModuleSdk.Devices.SdkInterfaces.IDeviceEEPROM.GetMaxNegativeCurrent | ( |  | ) |

Returns max negative current.

Returns

Implemented in MrEModuleSdk.Devices.Mre3.MrE3SdkComDeviceController.

## ◆ GetMaxPositiveCurrent()

int MrEModuleSdk.Devices.SdkInterfaces.IDeviceEEPROM.GetMaxPositiveCurrent | ( |  | ) |

Returns max positive current.

Returns

Implemented in MrEModuleSdk.Devices.Mre3.MrE3SdkComDeviceController.

## ◆ GetPartConfiguration()

int MrEModuleSdk.Devices.SdkInterfaces.IDeviceEEPROM.GetPartConfiguration | ( |  | ) |

Returns part configuration value.

Returns

Implemented in MrEModuleSdk.Devices.Mre3.MrE3SdkComDeviceController.

## ◆ GetPartConfigurationVersion()

int MrEModuleSdk.Devices.SdkInterfaces.IDeviceEEPROM.GetPartConfigurationVersion | ( |  | ) |

Returns part configuration version value.

Returns

Implemented in MrEModuleSdk.Devices.Mre3.MrE3SdkComDeviceController.

## ◆ LockMirrorEepromWriting()

void MrEModuleSdk.Devices.SdkInterfaces.IDeviceEEPROM.LockMirrorEepromWriting | ( |  | ) |

Locks mirror EEPROM writing.

Returns

Implemented in MrEModuleSdk.Devices.Mre3.MrE3SdkComDeviceController.

## ◆ ReparseMirrorEeprom()

void MrEModuleSdk.Devices.SdkInterfaces.IDeviceEEPROM.ReparseMirrorEeprom | ( |  | ) |

Reparse mirror EEPROM.

Returns

Implemented in MrEModuleSdk.Devices.Mre3.MrE3SdkComDeviceController.

## ◆ SetBytes()

void MrEModuleSdk.Devices.SdkInterfaces.IDeviceEEPROM.SetBytes | ( | int | index,
|  | byte[] | inputBytes )

Sets EEPROM bytes of the product.

Parameters

  index | Index of the start
  inputBytes | Bytes to be set

Returns

Implemented in MrEModuleSdk.Devices.Mre3.MrE3SdkComDeviceController.

## ◆ UnlockMirrorEepromWriting()

void MrEModuleSdk.Devices.SdkInterfaces.IDeviceEEPROM.UnlockMirrorEepromWriting | ( |  | ) |

Unlocks mirror EEPROM writing.

Returns

Implemented in MrEModuleSdk.Devices.Mre3.MrE3SdkComDeviceController.

The documentation for this interface was generated from the following file:

- C:/Users/jan.janda/Desktop/Mre3Documentation/IDeviceEEPROM.cs