\doxysection{Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+ITemperature\+Manager Interface Reference}
\hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager}{}\label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager}\index{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}}
\doxysubsubsection*{Public Member Functions}
\begin{DoxyCompactItemize}
\item 
int \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_afeef47c2bf0084c1c1f1a22a90146fea}{Read\+Device\+Temperature}} ()
\begin{DoxyCompactList}\small\item\em Returns device temperature. \end{DoxyCompactList}\item 
int \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_a0244a888e9eb01f71bfe9ff49f0f4dbb}{Read\+Proxy\+Temperature}} ()
\begin{DoxyCompactList}\small\item\em Returns board temperature. \end{DoxyCompactList}\item 
void \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_a5a023cf035c710e698554cf3d49d99b0}{Write\+Proxy\+Temperature\+Threshold}} (int temperature\+Threshold)
\begin{DoxyCompactList}\small\item\em Sets board temperature threshold. \end{DoxyCompactList}\item 
int \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_acb500dfb32437b2676711648e655154f}{Read\+Proxy\+Temperature\+Threshold}} ()
\begin{DoxyCompactList}\small\item\em Returns board temperature threshold. \end{DoxyCompactList}\item 
void \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_abd8cb27a9f7aee7c8bdc959128071c1f}{Write\+Device\+Temperature\+Threshold}} (int temperature\+Threshold)
\begin{DoxyCompactList}\small\item\em Sets device temperature threshold. \end{DoxyCompactList}\item 
int \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_ad3f2ffd5774b3212f4670c17511e304b}{Read\+Device\+Temperature\+Threshold}} ()
\begin{DoxyCompactList}\small\item\em Returns board temperature threshold. \end{DoxyCompactList}\item 
int \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_a8a99a10c7166d6808f433d1f5ceeb31e}{Read\+Board\+Output\+Stage\+Temperature}} ()
\begin{DoxyCompactList}\small\item\em Returns board output stage temperature. \end{DoxyCompactList}\item 
void \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_af6c9030e4e6776a3c864ccb6bde7a064}{Write\+Board\+Output\+Stage\+Temperature\+Threshold}} (int temperature\+Threshold)
\begin{DoxyCompactList}\small\item\em Sets board output stage temperature threshold. \end{DoxyCompactList}\item 
int \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_a17acf126a5b0646bc17522dd182e4421}{Read\+Board\+Output\+Stage\+Temperature\+Threshold}} ()
\begin{DoxyCompactList}\small\item\em Returns board output stage temperature threshold. \end{DoxyCompactList}\end{DoxyCompactItemize}


\doxysubsection{Member Function Documentation}
\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_a8a99a10c7166d6808f433d1f5ceeb31e}\index{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}!ReadBoardOutputStageTemperature@{ReadBoardOutputStageTemperature}}
\index{ReadBoardOutputStageTemperature@{ReadBoardOutputStageTemperature}!MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}}
\doxysubsubsection{\texorpdfstring{ReadBoardOutputStageTemperature()}{ReadBoardOutputStageTemperature()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_a8a99a10c7166d6808f433d1f5ceeb31e} 
int Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+ITemperature\+Manager.\+Read\+Board\+Output\+Stage\+Temperature (\begin{DoxyParamCaption}{}{}\end{DoxyParamCaption})}



Returns board output stage temperature. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}
\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_a17acf126a5b0646bc17522dd182e4421}\index{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}!ReadBoardOutputStageTemperatureThreshold@{ReadBoardOutputStageTemperatureThreshold}}
\index{ReadBoardOutputStageTemperatureThreshold@{ReadBoardOutputStageTemperatureThreshold}!MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}}
\doxysubsubsection{\texorpdfstring{ReadBoardOutputStageTemperatureThreshold()}{ReadBoardOutputStageTemperatureThreshold()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_a17acf126a5b0646bc17522dd182e4421} 
int Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+ITemperature\+Manager.\+Read\+Board\+Output\+Stage\+Temperature\+Threshold (\begin{DoxyParamCaption}{}{}\end{DoxyParamCaption})}



Returns board output stage temperature threshold. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}
\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_afeef47c2bf0084c1c1f1a22a90146fea}\index{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}!ReadDeviceTemperature@{ReadDeviceTemperature}}
\index{ReadDeviceTemperature@{ReadDeviceTemperature}!MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}}
\doxysubsubsection{\texorpdfstring{ReadDeviceTemperature()}{ReadDeviceTemperature()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_afeef47c2bf0084c1c1f1a22a90146fea} 
int Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+ITemperature\+Manager.\+Read\+Device\+Temperature (\begin{DoxyParamCaption}{}{}\end{DoxyParamCaption})}



Returns device temperature. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}
\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_ad3f2ffd5774b3212f4670c17511e304b}\index{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}!ReadDeviceTemperatureThreshold@{ReadDeviceTemperatureThreshold}}
\index{ReadDeviceTemperatureThreshold@{ReadDeviceTemperatureThreshold}!MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}}
\doxysubsubsection{\texorpdfstring{ReadDeviceTemperatureThreshold()}{ReadDeviceTemperatureThreshold()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_ad3f2ffd5774b3212f4670c17511e304b} 
int Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+ITemperature\+Manager.\+Read\+Device\+Temperature\+Threshold (\begin{DoxyParamCaption}{}{}\end{DoxyParamCaption})}



Returns board temperature threshold. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}
\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_a0244a888e9eb01f71bfe9ff49f0f4dbb}\index{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}!ReadProxyTemperature@{ReadProxyTemperature}}
\index{ReadProxyTemperature@{ReadProxyTemperature}!MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}}
\doxysubsubsection{\texorpdfstring{ReadProxyTemperature()}{ReadProxyTemperature()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_a0244a888e9eb01f71bfe9ff49f0f4dbb} 
int Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+ITemperature\+Manager.\+Read\+Proxy\+Temperature (\begin{DoxyParamCaption}{}{}\end{DoxyParamCaption})}



Returns board temperature. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}
\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_acb500dfb32437b2676711648e655154f}\index{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}!ReadProxyTemperatureThreshold@{ReadProxyTemperatureThreshold}}
\index{ReadProxyTemperatureThreshold@{ReadProxyTemperatureThreshold}!MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}}
\doxysubsubsection{\texorpdfstring{ReadProxyTemperatureThreshold()}{ReadProxyTemperatureThreshold()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_acb500dfb32437b2676711648e655154f} 
int Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+ITemperature\+Manager.\+Read\+Proxy\+Temperature\+Threshold (\begin{DoxyParamCaption}{}{}\end{DoxyParamCaption})}



Returns board temperature threshold. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}
\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_af6c9030e4e6776a3c864ccb6bde7a064}\index{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}!WriteBoardOutputStageTemperatureThreshold@{WriteBoardOutputStageTemperatureThreshold}}
\index{WriteBoardOutputStageTemperatureThreshold@{WriteBoardOutputStageTemperatureThreshold}!MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}}
\doxysubsubsection{\texorpdfstring{WriteBoardOutputStageTemperatureThreshold()}{WriteBoardOutputStageTemperatureThreshold()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_af6c9030e4e6776a3c864ccb6bde7a064} 
void Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+ITemperature\+Manager.\+Write\+Board\+Output\+Stage\+Temperature\+Threshold (\begin{DoxyParamCaption}\item[{int}]{temperature\+Threshold}{}\end{DoxyParamCaption})}



Sets board output stage temperature threshold. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}
\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_abd8cb27a9f7aee7c8bdc959128071c1f}\index{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}!WriteDeviceTemperatureThreshold@{WriteDeviceTemperatureThreshold}}
\index{WriteDeviceTemperatureThreshold@{WriteDeviceTemperatureThreshold}!MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}}
\doxysubsubsection{\texorpdfstring{WriteDeviceTemperatureThreshold()}{WriteDeviceTemperatureThreshold()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_abd8cb27a9f7aee7c8bdc959128071c1f} 
void Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+ITemperature\+Manager.\+Write\+Device\+Temperature\+Threshold (\begin{DoxyParamCaption}\item[{int}]{temperature\+Threshold}{}\end{DoxyParamCaption})}



Sets device temperature threshold. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}
\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_a5a023cf035c710e698554cf3d49d99b0}\index{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}!WriteProxyTemperatureThreshold@{WriteProxyTemperatureThreshold}}
\index{WriteProxyTemperatureThreshold@{WriteProxyTemperatureThreshold}!MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.ITemperatureManager}}
\doxysubsubsection{\texorpdfstring{WriteProxyTemperatureThreshold()}{WriteProxyTemperatureThreshold()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_temperature_manager_a5a023cf035c710e698554cf3d49d99b0} 
void Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+ITemperature\+Manager.\+Write\+Proxy\+Temperature\+Threshold (\begin{DoxyParamCaption}\item[{int}]{temperature\+Threshold}{}\end{DoxyParamCaption})}



Sets board temperature threshold. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


The documentation for this interface was generated from the following file\+:\begin{DoxyCompactItemize}
\item 
C\+:/\+Users/jan.\+janda/\+Desktop/\+Mre3\+Documentation/\mbox{\hyperlink{_i_temperature_manager_8cs}{ITemperature\+Manager.\+cs}}\end{DoxyCompactItemize}
