MR-E-2 SDK

Public Member Functions | Properties | List of all members
MrE2ModuleSdk.Device.IInputStage Interface Reference
Inheritance diagram for MrE2ModuleSdk.Device.IInputStage:

## Public Member Functions
EmrE2InputStageSystems | ReadActiveSystem (EAxis axis)
| Returns active input system of the axis. More...
void | ChangeActiveSystem (EAxis axis, EmrE2InputStageSystems selectedInputStageSystem)
| Changes active input system of the axis. More...

## Properties
IStaticValue | StaticValue`[get]`
IAnalogInput | AnalogInput`[get]`
ISignalGenerator | SignalGenerator`[get]`
IArbitraryVector | ArbitraryVector`[get]`

## Member Function Documentation

## ◆ ChangeActiveSystem()

void MrE2ModuleSdk.Device.IInputStage.ChangeActiveSystem | ( | EAxis | axis,
|  | EmrE2InputStageSystems | selectedInputStageSystem
| ) |  |

Changes active input system of the axis.

Returns

Implemented in MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController.

## ◆ ReadActiveSystem()

EmrE2InputStageSystems MrE2ModuleSdk.Device.IInputStage.ReadActiveSystem | ( | EAxis | axis | ) |

Returns active input system of the axis.

Returns

Implemented in MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController.

The documentation for this interface was generated from the following file:

- Device/MrE2SdkComDeviceController.cs