MR-E-2 SDK

Public Member Functions | List of all members
MrE2ModuleSdk.Device.IAnalogInput Interface Reference
Inheritance diagram for MrE2ModuleSdk.Device.IAnalogInput:

## Public Member Functions
ushort | ReadAdcRawValue (EAxis axis)
| Returns converted ADC raw value. More...
EUnitType | ReadActiveInputType (EAxis axis)
| Returns active analog input type. Determined by active control stage system. More...

## Member Function Documentation

## ◆ ReadActiveInputType()

EUnitType MrE2ModuleSdk.Device.IAnalogInput.ReadActiveInputType | ( | EAxis | axis | ) |

Returns active analog input type. Determined by active control stage system.

Returns

Implemented in MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController.

## ◆ ReadAdcRawValue()

ushort MrE2ModuleSdk.Device.IAnalogInput.ReadAdcRawValue | ( | EAxis | axis | ) |

Returns converted ADC raw value.

Returns

Implemented in MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController.

The documentation for this interface was generated from the following file:

- Device/MrE2SdkComDeviceController.cs