\doxysection{Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+Input\+Stage.\+IAnalog\+Input Interface Reference}
\hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_analog_input}{}\label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_analog_input}\index{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IAnalogInput@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IAnalogInput}}
Inheritance diagram for Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+Input\+Stage.\+IAnalog\+Input\+:\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[height=2.000000cm]{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_analog_input}
\end{center}
\end{figure}
\doxysubsubsection*{Public Member Functions}
\begin{DoxyCompactItemize}
\item 
ushort \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_analog_input_ac73af79d227ee2fb04f1fefd5ec8e110}{Read\+Adc\+Raw\+Value}} (EAxis axis)
\begin{DoxyCompactList}\small\item\em Returns converted ADC raw value. ~\newline
 \end{DoxyCompactList}\item 
EUnit\+Type \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_analog_input_a5e04861578c805cb3f839eb69a7c179c}{Read\+Active\+Input\+Type}} (EAxis axis)
\begin{DoxyCompactList}\small\item\em Returns active analog input type. Determined by active control stage system. ~\newline
 \end{DoxyCompactList}\end{DoxyCompactItemize}


\doxysubsection{Member Function Documentation}
\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_analog_input_a5e04861578c805cb3f839eb69a7c179c}\index{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IAnalogInput@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IAnalogInput}!ReadActiveInputType@{ReadActiveInputType}}
\index{ReadActiveInputType@{ReadActiveInputType}!MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IAnalogInput@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IAnalogInput}}
\doxysubsubsection{\texorpdfstring{ReadActiveInputType()}{ReadActiveInputType()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_analog_input_a5e04861578c805cb3f839eb69a7c179c} 
EUnit\+Type Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+Input\+Stage.\+IAnalog\+Input.\+Read\+Active\+Input\+Type (\begin{DoxyParamCaption}\item[{EAxis}]{axis}{}\end{DoxyParamCaption})}



Returns active analog input type. Determined by active control stage system. ~\newline
 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_a732e8505b0df675a84d16d342546bede}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_analog_input_ac73af79d227ee2fb04f1fefd5ec8e110}\index{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IAnalogInput@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IAnalogInput}!ReadAdcRawValue@{ReadAdcRawValue}}
\index{ReadAdcRawValue@{ReadAdcRawValue}!MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IAnalogInput@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IAnalogInput}}
\doxysubsubsection{\texorpdfstring{ReadAdcRawValue()}{ReadAdcRawValue()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_analog_input_ac73af79d227ee2fb04f1fefd5ec8e110} 
ushort Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+Input\+Stage.\+IAnalog\+Input.\+Read\+Adc\+Raw\+Value (\begin{DoxyParamCaption}\item[{EAxis}]{axis}{}\end{DoxyParamCaption})}



Returns converted ADC raw value. ~\newline
 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_ab582a801957790cf1910d2feee771406}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.



The documentation for this interface was generated from the following file\+:\begin{DoxyCompactItemize}
\item 
C\+:/\+Users/jan.\+janda/\+Desktop/\+Mre3\+Documentation/\+Signal\+Flow\+Manager/\+Input\+Stage/\mbox{\hyperlink{_i_analog_input_8cs}{IAnalog\+Input.\+cs}}\end{DoxyCompactItemize}
