MR-E-2 SDK

Public Member Functions | List of all members
MrE2ModuleSdk.Device.IBoardEeprom Interface Reference
Inheritance diagram for MrE2ModuleSdk.Device.IBoardEeprom:

## Public Member Functions
void | SetBytes (int index, byte[] inputBytes)
| Sets board EEPROM bytes starting at index provided as parameter. More...
byte[] | GetBytes (int index, int length)
| Returns board EEPROM bytes starting at index provided as parameter. More...
void | LockWriting ()
| Locks board EEPROM writing. More...
void | UnlockWriting ()
| Unlocks board EEPROM writing. More...

## Member Function Documentation

## ◆ GetBytes()

byte [] MrE2ModuleSdk.Device.IBoardEeprom.GetBytes | ( | int | index,
|  | int | length
| ) |  |

Returns board EEPROM bytes starting at index provided as parameter.

Returns

Implemented in MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController.

## ◆ LockWriting()

void MrE2ModuleSdk.Device.IBoardEeprom.LockWriting | ( |  | ) |

Locks board EEPROM writing.

Returns

Implemented in MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController.

## ◆ SetBytes()

void MrE2ModuleSdk.Device.IBoardEeprom.SetBytes | ( | int | index,
|  | byte[] | inputBytes
| ) |  |

Sets board EEPROM bytes starting at index provided as parameter.

Returns

Implemented in MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController.

## ◆ UnlockWriting()

void MrE2ModuleSdk.Device.IBoardEeprom.UnlockWriting | ( |  | ) |

Unlocks board EEPROM writing.

Returns

Implemented in MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController.

The documentation for this interface was generated from the following file:

- Device/MrE2SdkComDeviceController.cs