\doxysection{Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+Input\+Stage.\+IStatic\+Value Interface Reference}
\hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value}{}\label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value}\index{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue}}
Inheritance diagram for Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+Input\+Stage.\+IStatic\+Value\+:\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[height=2.000000cm]{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value}
\end{center}
\end{figure}
\doxysubsubsection*{Public Member Functions}
\begin{DoxyCompactItemize}
\item 
float \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_ab6570573c9920f4863b36f7be22783c4}{Read\+Current}} (EAxis axis)
\begin{DoxyCompactList}\small\item\em Returns static input in amperes. Range is from -\/0.\+7 to 0.\+7. \end{DoxyCompactList}\item 
void \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_a25872c2905db8b898e54cc46f01a63cd}{Write\+Current}} (EAxis axis, float value)
\begin{DoxyCompactList}\small\item\em Sets static input in amperes. Range is from -\/0.\+7 to 0.\+7. ~\newline
 \end{DoxyCompactList}\item 
float \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_a5993ae144ed500edb9c55783b536a355}{Read\+Angle}} (EAxis axis)
\begin{DoxyCompactList}\small\item\em Returns static input in XY coordinates. Range is from -\/1.\+0 to 1.\+0. \end{DoxyCompactList}\item 
void \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_ac1f7f3fce6e3b99f46e0916411518d2a}{Write\+Angle}} (EAxis axis, float value)
\begin{DoxyCompactList}\small\item\em Sets static input in XY coordinates. Range is from -\/1.\+0 to 1.\+0. \end{DoxyCompactList}\item 
float \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_aaa1fbd717d329fa236ff047cd240a67f}{Read\+Optical\+Feedback}} (EAxis axis)
\begin{DoxyCompactList}\small\item\em Returns static input in OF. Range differs for each mirror. \end{DoxyCompactList}\item 
void \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_a465f55c04ca3dda1c5104c7fe6f0bc8a}{Write\+Optical\+Feedback}} (EAxis axis, float value)
\begin{DoxyCompactList}\small\item\em Sets static input in OF. Range differs for each mirror. \end{DoxyCompactList}\item 
EUnit\+Type \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_a81e6ecb506df971f5ba3c7ca26ab547b}{Read\+Active\+Static\+Input\+Type}} (EAxis axis)
\begin{DoxyCompactList}\small\item\em Returns active static input type. Determined by active control stage system. ~\newline
 \end{DoxyCompactList}\end{DoxyCompactItemize}


\doxysubsection{Member Function Documentation}
\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_a81e6ecb506df971f5ba3c7ca26ab547b}\index{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue}!ReadActiveStaticInputType@{ReadActiveStaticInputType}}
\index{ReadActiveStaticInputType@{ReadActiveStaticInputType}!MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue}}
\doxysubsubsection{\texorpdfstring{ReadActiveStaticInputType()}{ReadActiveStaticInputType()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_a81e6ecb506df971f5ba3c7ca26ab547b} 
EUnit\+Type Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+Input\+Stage.\+IStatic\+Value.\+Read\+Active\+Static\+Input\+Type (\begin{DoxyParamCaption}\item[{EAxis}]{axis}{}\end{DoxyParamCaption})}



Returns active static input type. Determined by active control stage system. ~\newline
 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_adc1d5a2674d836ab842198c28d0660ee}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_a5993ae144ed500edb9c55783b536a355}\index{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue}!ReadAngle@{ReadAngle}}
\index{ReadAngle@{ReadAngle}!MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue}}
\doxysubsubsection{\texorpdfstring{ReadAngle()}{ReadAngle()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_a5993ae144ed500edb9c55783b536a355} 
float Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+Input\+Stage.\+IStatic\+Value.\+Read\+Angle (\begin{DoxyParamCaption}\item[{EAxis}]{axis}{}\end{DoxyParamCaption})}



Returns static input in XY coordinates. Range is from -\/1.\+0 to 1.\+0. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_acf423480e2896ebdca6a51531fd3c3dd}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_ab6570573c9920f4863b36f7be22783c4}\index{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue}!ReadCurrent@{ReadCurrent}}
\index{ReadCurrent@{ReadCurrent}!MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue}}
\doxysubsubsection{\texorpdfstring{ReadCurrent()}{ReadCurrent()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_ab6570573c9920f4863b36f7be22783c4} 
float Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+Input\+Stage.\+IStatic\+Value.\+Read\+Current (\begin{DoxyParamCaption}\item[{EAxis}]{axis}{}\end{DoxyParamCaption})}



Returns static input in amperes. Range is from -\/0.\+7 to 0.\+7. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_afc1a9d671a9ee22eaf267b96b996c3c5}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_aaa1fbd717d329fa236ff047cd240a67f}\index{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue}!ReadOpticalFeedback@{ReadOpticalFeedback}}
\index{ReadOpticalFeedback@{ReadOpticalFeedback}!MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue}}
\doxysubsubsection{\texorpdfstring{ReadOpticalFeedback()}{ReadOpticalFeedback()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_aaa1fbd717d329fa236ff047cd240a67f} 
float Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+Input\+Stage.\+IStatic\+Value.\+Read\+Optical\+Feedback (\begin{DoxyParamCaption}\item[{EAxis}]{axis}{}\end{DoxyParamCaption})}



Returns static input in OF. Range differs for each mirror. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_a6bc0dfb8b8ff5c990e758e4257f0313a}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_ac1f7f3fce6e3b99f46e0916411518d2a}\index{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue}!WriteAngle@{WriteAngle}}
\index{WriteAngle@{WriteAngle}!MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue}}
\doxysubsubsection{\texorpdfstring{WriteAngle()}{WriteAngle()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_ac1f7f3fce6e3b99f46e0916411518d2a} 
void Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+Input\+Stage.\+IStatic\+Value.\+Write\+Angle (\begin{DoxyParamCaption}\item[{EAxis}]{axis}{, }\item[{float}]{value}{}\end{DoxyParamCaption})}



Sets static input in XY coordinates. Range is from -\/1.\+0 to 1.\+0. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_a1040edbf70491eb3fd50686598d7ca5c}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_a25872c2905db8b898e54cc46f01a63cd}\index{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue}!WriteCurrent@{WriteCurrent}}
\index{WriteCurrent@{WriteCurrent}!MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue}}
\doxysubsubsection{\texorpdfstring{WriteCurrent()}{WriteCurrent()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_a25872c2905db8b898e54cc46f01a63cd} 
void Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+Input\+Stage.\+IStatic\+Value.\+Write\+Current (\begin{DoxyParamCaption}\item[{EAxis}]{axis}{, }\item[{float}]{value}{}\end{DoxyParamCaption})}



Sets static input in amperes. Range is from -\/0.\+7 to 0.\+7. ~\newline
 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_af363b4b9f5cfb43548df8170438fbdef}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_a465f55c04ca3dda1c5104c7fe6f0bc8a}\index{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue}!WriteOpticalFeedback@{WriteOpticalFeedback}}
\index{WriteOpticalFeedback@{WriteOpticalFeedback}!MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue@{MrEModuleSdk.Devices.SdkInterfaces.SignalFlowManager.InputStage.IStaticValue}}
\doxysubsubsection{\texorpdfstring{WriteOpticalFeedback()}{WriteOpticalFeedback()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_signal_flow_manager_1_1_input_stage_1_1_i_static_value_a465f55c04ca3dda1c5104c7fe6f0bc8a} 
void Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+Signal\+Flow\+Manager.\+Input\+Stage.\+IStatic\+Value.\+Write\+Optical\+Feedback (\begin{DoxyParamCaption}\item[{EAxis}]{axis}{, }\item[{float}]{value}{}\end{DoxyParamCaption})}



Sets static input in OF. Range differs for each mirror. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_aeb80adfb83a03aaeb96f64b7b516fb31}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.



The documentation for this interface was generated from the following file\+:\begin{DoxyCompactItemize}
\item 
C\+:/\+Users/jan.\+janda/\+Desktop/\+Mre3\+Documentation/\+Signal\+Flow\+Manager/\+Input\+Stage/\mbox{\hyperlink{_i_static_value_8cs}{IStatic\+Value.\+cs}}\end{DoxyCompactItemize}
