MR-E-2 SDK

### - r -

- ReadActiveInputType() : MrE2ModuleSdk.Device.IAnalogInput , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadActiveStaticInputType() : MrE2ModuleSdk.Device.IStaticValue , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadActiveSystem() : MrE2ModuleSdk.Device.IControlModeStage , MrE2ModuleSdk.Device.IInputStage , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadActualCurrent() : MrE2ModuleSdk.Device.ILinearOutput , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadActualOutputAngle() : MrE2ModuleSdk.Device.IOpticalFeedbackManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadActualOutputOpticalFeedback() : MrE2ModuleSdk.Device.IOpticalFeedbackManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadAdcRawValue() : MrE2ModuleSdk.Device.IAnalogInput , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadAmplitude() : MrE2ModuleSdk.Device.ISignalGenerator , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadAngle() : MrE2ModuleSdk.Device.IStaticValue , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadAverageLimitPeriod() : MrE2ModuleSdk.Device.ILinearOutput , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadAverageLimitSum() : MrE2ModuleSdk.Device.ILinearOutput , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadBoardEepromDumpSize() : MrE2ModuleSdk.Device.IMiscellaneousFeatures , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadBoardTemperature() : MrE2ModuleSdk.Device.ITemperatureManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadBoardTemperatureThreshold() : MrE2ModuleSdk.Device.ITemperatureManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadChannelNumber() : MrE2ModuleSdk.Device.ILinearOutput , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadCooldownPeriod() : MrE2ModuleSdk.Device.ILinearOutput , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadCurrent() : MrE2ModuleSdk.Device.IStaticValue , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadCurrentLimit() : MrE2ModuleSdk.Device.ILinearOutput , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadCutOffFrequency() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadCycles() : MrE2ModuleSdk.Device.IArbitraryVector , MrE2ModuleSdk.Device.ISignalGenerator , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadDataSize() : MrE2ModuleSdk.Device.IVectorAdapter , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadDerivativeGainConstantTerm() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadDerivativeGainLinearTermMultiplier() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadDerivativeGainQuadraticTermMultiplier() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadDerivativeTermFilterEnabled() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadDesiredSetPoint() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadDeviceEepromDumpSize() : MrE2ModuleSdk.Device.IMiscellaneousFeatures , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadDeviceTemperature() : MrE2ModuleSdk.Device.ITemperatureManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadDeviceTemperatureThreshold() : MrE2ModuleSdk.Device.ITemperatureManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadDGain() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadDutyCycles() : MrE2ModuleSdk.Device.ISignalGenerator , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadErrorFlag() : MrE2ModuleSdk.Device.IVectorAdapter , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadErrorRegisterId() : MrE2ModuleSdk.Device.ISnapshotManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadErrorSystemId() : MrE2ModuleSdk.Device.ISnapshotManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadErrorValue() : MrE2ModuleSdk.Device.ISnapshotManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadExternalTrigger() : MrE2ModuleSdk.Device.IArbitraryVector , MrE2ModuleSdk.Device.ISignalGenerator , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadFilteredPhotoDiodePd0() : MrE2ModuleSdk.Device.IOpticalFeedbackManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadFilteredPhotoDiodePd1() : MrE2ModuleSdk.Device.IOpticalFeedbackManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadFilteredPhotoDiodePd2() : MrE2ModuleSdk.Device.IOpticalFeedbackManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadFilteredPhotoDiodePd3() : MrE2ModuleSdk.Device.IOpticalFeedbackManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadFrequency() : MrE2ModuleSdk.Device.ISignalGenerator , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadGainSchedulingVariable() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadI2CReadPointer0Address() : MrE2ModuleSdk.Device.II2C , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadI2CReadPointer1Address() : MrE2ModuleSdk.Device.II2C , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadIGain() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadIntegralGainConstantTerm() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadIntegralGainLinearTermMultiplier() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadIntegralGainQuadraticTermMultiplier() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadLoggedRegisterAddress() : MrE2ModuleSdk.Device.ILogger , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadLoggerMaximumSamplingFrequency() : MrE2ModuleSdk.Device.ILogger , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadLoggerMinimumSamplingFrequency() : MrE2ModuleSdk.Device.ILogger , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadLoggerRegisterLog() : MrE2ModuleSdk.Device.ILogger , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadLoggerSamplingRate() : MrE2ModuleSdk.Device.ILogger , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadMaximumIntegral() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadMaximumOutput() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadMaximumSamplingRate() : MrE2ModuleSdk.Device.IArbitraryVector , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadMinimumIntegral() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadMinimumOutput() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadMinimumSamplingRate() : MrE2ModuleSdk.Device.IArbitraryVector , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadMirrorLedIntensity() : MrE2ModuleSdk.Device.IMiscellaneousFeatures , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadNumberOfAvailableSnapshots() : MrE2ModuleSdk.Device.ISnapshotManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadOffset() : MrE2ModuleSdk.Device.IOffsetAndScale , MrE2ModuleSdk.Device.ISignalGenerator , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadOpticalFeedback() : MrE2ModuleSdk.Device.IStaticValue , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadPGain() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadPhaseDelay() : MrE2ModuleSdk.Device.ISignalGenerator , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadProportionalGainConstantTerm() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadProportionalGainLinearTermMultiplier() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadProportionalGainQuadraticTermMultiplier() : MrE2ModuleSdk.Device.IAnglePid , MrE2ModuleSdk.Device.IOpticalFeedbackPid
- ReadRawPhotoDiodePd0() : MrE2ModuleSdk.Device.IOpticalFeedbackManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadRawPhotoDiodePd1() : MrE2ModuleSdk.Device.IOpticalFeedbackManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadRawPhotoDiodePd2() : MrE2ModuleSdk.Device.IOpticalFeedbackManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadRawPhotoDiodePd3() : MrE2ModuleSdk.Device.IOpticalFeedbackManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadSampleRate() : MrE2ModuleSdk.Device.IArbitraryVector , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadScale() : MrE2ModuleSdk.Device.IOffsetAndScale , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadShape() : MrE2ModuleSdk.Device.ISignalGenerator , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadSignalGeneratorValues() : MrE2ModuleSdk.Device.ISignalGenerator , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadSpiReadPointer0Address() : MrE2ModuleSdk.Device.ISpi , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadSpiReadPointer1Address() : MrE2ModuleSdk.Device.ISpi , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadStabilityCriterionPositionParameterA() : MrE2ModuleSdk.Device.IOpticalFeedbackManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadStabilityCriterionPositionParameterB() : MrE2ModuleSdk.Device.IOpticalFeedbackManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadStabilityCriterionVelocityParameterA() : MrE2ModuleSdk.Device.IOpticalFeedbackManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadStabilityCriterionVelocityParameterB() : MrE2ModuleSdk.Device.IOpticalFeedbackManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadStartupSnapshotNumber() : MrE2ModuleSdk.Device.ISnapshotManager , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadSystemTick() : MrE2ModuleSdk.Device.ISpi , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadUnitType() : MrE2ModuleSdk.Device.IArbitraryVector , MrE2ModuleSdk.Device.ISignalGenerator , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadVector() : MrE2ModuleSdk.Device.IVectorAdapter , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadVectorAddress() : MrE2ModuleSdk.Device.IVectorAdapter , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadVectorData() : MrE2ModuleSdk.Device.IVectorAdapter , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadVectorIndex() : MrE2ModuleSdk.Device.IVectorAdapter , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReadVectorValues() : MrE2ModuleSdk.Device.IArbitraryVector
- ReaI2CErrorResponse0() : MrE2ModuleSdk.Device.II2C , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReaI2CErrorResponse1() : MrE2ModuleSdk.Device.II2C , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- Reconnect() : MrE2ModuleSdk.Device.IMrE2ForMr15Dash30SdkComDeviceController , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ReparseMirrorEeprom() : MrE2ModuleSdk.Device.IDeviceEeprom , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ResetErrorFlags() : MrE2ModuleSdk.Device.IStatus , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController
- ResetFirmware() : MrE2ModuleSdk.Device.IMiscellaneousFeatures , MrE2ModuleSdk.Device.MrE2ForMr15Dash30SdkComDeviceController