\doxysection{Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+IMre3\+Temperature\+Manager Interface Reference}
\hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager}{}\label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager}\index{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}}
Inheritance diagram for Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+IMre3\+Temperature\+Manager\+:\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[height=2.000000cm]{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager}
\end{center}
\end{figure}
\doxysubsubsection*{Public Member Functions}
\begin{DoxyCompactItemize}
\item 
float \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a31574255a21abe803f88bfd1d97ea868}{Read\+Device\+Temperature}} ()
\begin{DoxyCompactList}\small\item\em Returns device temperature. \end{DoxyCompactList}\item 
float \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a6075ebf938ba897d453397e0dcff7286}{Read\+Proxy\+Temperature}} ()
\begin{DoxyCompactList}\small\item\em Returns board temperature. \end{DoxyCompactList}\item 
void \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_aad9955a68a1b6588e0bd8e335eeae67c}{Write\+Proxy\+Temperature\+Threshold}} (float temperature\+Threshold)
\begin{DoxyCompactList}\small\item\em Sets board temperature threshold. \end{DoxyCompactList}\item 
float \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a8219267708db408e48dc4b1f5be286ed}{Read\+Proxy\+Temperature\+Threshold}} ()
\begin{DoxyCompactList}\small\item\em Returns board temperature threshold. \end{DoxyCompactList}\item 
void \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a1000af1be4fe1de7cef780f356e459bd}{Write\+Device\+Temperature\+Threshold}} (float temperature\+Threshold)
\begin{DoxyCompactList}\small\item\em Sets device temperature threshold. \end{DoxyCompactList}\item 
float \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_ab92fad225d74332efb8275026ae3c4dd}{Read\+Device\+Temperature\+Threshold}} ()
\begin{DoxyCompactList}\small\item\em Returns board temperature threshold. \end{DoxyCompactList}\item 
float \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a8102d7c48b9c8517c32bf4e07a50e903}{Read\+Board\+Output\+Stage\+Temperature}} ()
\begin{DoxyCompactList}\small\item\em Returns board output stage temperature. \end{DoxyCompactList}\item 
void \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a445057a1873694d80112326fa869878f}{Write\+Board\+Output\+Stage\+Temperature\+Threshold}} (float temperature\+Threshold)
\begin{DoxyCompactList}\small\item\em Sets board output stage temperature threshold. \end{DoxyCompactList}\item 
float \mbox{\hyperlink{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a2e543cc9654dc0525c246440b25387d1}{Read\+Board\+Output\+Stage\+Temperature\+Threshold}} ()
\begin{DoxyCompactList}\small\item\em Returns board output stage temperature threshold. \end{DoxyCompactList}\end{DoxyCompactItemize}


\doxysubsection{Member Function Documentation}
\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a8102d7c48b9c8517c32bf4e07a50e903}\index{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}!ReadBoardOutputStageTemperature@{ReadBoardOutputStageTemperature}}
\index{ReadBoardOutputStageTemperature@{ReadBoardOutputStageTemperature}!MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}}
\doxysubsubsection{\texorpdfstring{ReadBoardOutputStageTemperature()}{ReadBoardOutputStageTemperature()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a8102d7c48b9c8517c32bf4e07a50e903} 
float Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+IMre3\+Temperature\+Manager.\+Read\+Board\+Output\+Stage\+Temperature (\begin{DoxyParamCaption}{}{}\end{DoxyParamCaption})}



Returns board output stage temperature. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_a08ffad78aa0d45a50994a145e414d695}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a2e543cc9654dc0525c246440b25387d1}\index{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}!ReadBoardOutputStageTemperatureThreshold@{ReadBoardOutputStageTemperatureThreshold}}
\index{ReadBoardOutputStageTemperatureThreshold@{ReadBoardOutputStageTemperatureThreshold}!MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}}
\doxysubsubsection{\texorpdfstring{ReadBoardOutputStageTemperatureThreshold()}{ReadBoardOutputStageTemperatureThreshold()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a2e543cc9654dc0525c246440b25387d1} 
float Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+IMre3\+Temperature\+Manager.\+Read\+Board\+Output\+Stage\+Temperature\+Threshold (\begin{DoxyParamCaption}{}{}\end{DoxyParamCaption})}



Returns board output stage temperature threshold. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_a3d227c8251bc85ea599a721ebb563f52}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a31574255a21abe803f88bfd1d97ea868}\index{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}!ReadDeviceTemperature@{ReadDeviceTemperature}}
\index{ReadDeviceTemperature@{ReadDeviceTemperature}!MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}}
\doxysubsubsection{\texorpdfstring{ReadDeviceTemperature()}{ReadDeviceTemperature()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a31574255a21abe803f88bfd1d97ea868} 
float Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+IMre3\+Temperature\+Manager.\+Read\+Device\+Temperature (\begin{DoxyParamCaption}{}{}\end{DoxyParamCaption})}



Returns device temperature. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_a636c7943d36fdfef46f2ca23855eda1b}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_ab92fad225d74332efb8275026ae3c4dd}\index{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}!ReadDeviceTemperatureThreshold@{ReadDeviceTemperatureThreshold}}
\index{ReadDeviceTemperatureThreshold@{ReadDeviceTemperatureThreshold}!MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}}
\doxysubsubsection{\texorpdfstring{ReadDeviceTemperatureThreshold()}{ReadDeviceTemperatureThreshold()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_ab92fad225d74332efb8275026ae3c4dd} 
float Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+IMre3\+Temperature\+Manager.\+Read\+Device\+Temperature\+Threshold (\begin{DoxyParamCaption}{}{}\end{DoxyParamCaption})}



Returns board temperature threshold. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_ad0e7363b75f7bf355fff4daa416986de}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a6075ebf938ba897d453397e0dcff7286}\index{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}!ReadProxyTemperature@{ReadProxyTemperature}}
\index{ReadProxyTemperature@{ReadProxyTemperature}!MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}}
\doxysubsubsection{\texorpdfstring{ReadProxyTemperature()}{ReadProxyTemperature()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a6075ebf938ba897d453397e0dcff7286} 
float Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+IMre3\+Temperature\+Manager.\+Read\+Proxy\+Temperature (\begin{DoxyParamCaption}{}{}\end{DoxyParamCaption})}



Returns board temperature. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_a93591ec9532f5d9674272748d9230684}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a8219267708db408e48dc4b1f5be286ed}\index{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}!ReadProxyTemperatureThreshold@{ReadProxyTemperatureThreshold}}
\index{ReadProxyTemperatureThreshold@{ReadProxyTemperatureThreshold}!MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}}
\doxysubsubsection{\texorpdfstring{ReadProxyTemperatureThreshold()}{ReadProxyTemperatureThreshold()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a8219267708db408e48dc4b1f5be286ed} 
float Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+IMre3\+Temperature\+Manager.\+Read\+Proxy\+Temperature\+Threshold (\begin{DoxyParamCaption}{}{}\end{DoxyParamCaption})}



Returns board temperature threshold. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_acb177744219d23a7257296f4530a7a5d}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a445057a1873694d80112326fa869878f}\index{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}!WriteBoardOutputStageTemperatureThreshold@{WriteBoardOutputStageTemperatureThreshold}}
\index{WriteBoardOutputStageTemperatureThreshold@{WriteBoardOutputStageTemperatureThreshold}!MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}}
\doxysubsubsection{\texorpdfstring{WriteBoardOutputStageTemperatureThreshold()}{WriteBoardOutputStageTemperatureThreshold()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a445057a1873694d80112326fa869878f} 
void Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+IMre3\+Temperature\+Manager.\+Write\+Board\+Output\+Stage\+Temperature\+Threshold (\begin{DoxyParamCaption}\item[{float}]{temperature\+Threshold}{}\end{DoxyParamCaption})}



Sets board output stage temperature threshold. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_a4de11b479757cd3bc17902a5ba85fddf}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a1000af1be4fe1de7cef780f356e459bd}\index{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}!WriteDeviceTemperatureThreshold@{WriteDeviceTemperatureThreshold}}
\index{WriteDeviceTemperatureThreshold@{WriteDeviceTemperatureThreshold}!MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}}
\doxysubsubsection{\texorpdfstring{WriteDeviceTemperatureThreshold()}{WriteDeviceTemperatureThreshold()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_a1000af1be4fe1de7cef780f356e459bd} 
void Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+IMre3\+Temperature\+Manager.\+Write\+Device\+Temperature\+Threshold (\begin{DoxyParamCaption}\item[{float}]{temperature\+Threshold}{}\end{DoxyParamCaption})}



Sets device temperature threshold. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_a246ba82dfa8731184f9c55eb103dfaef}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.

\Hypertarget{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_aad9955a68a1b6588e0bd8e335eeae67c}\index{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}!WriteProxyTemperatureThreshold@{WriteProxyTemperatureThreshold}}
\index{WriteProxyTemperatureThreshold@{WriteProxyTemperatureThreshold}!MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager@{MrEModuleSdk.Devices.SdkInterfaces.IMre3TemperatureManager}}
\doxysubsubsection{\texorpdfstring{WriteProxyTemperatureThreshold()}{WriteProxyTemperatureThreshold()}}
{\footnotesize\ttfamily \label{interface_mr_e_module_sdk_1_1_devices_1_1_sdk_interfaces_1_1_i_mre3_temperature_manager_aad9955a68a1b6588e0bd8e335eeae67c} 
void Mr\+EModule\+Sdk.\+Devices.\+Sdk\+Interfaces.\+IMre3\+Temperature\+Manager.\+Write\+Proxy\+Temperature\+Threshold (\begin{DoxyParamCaption}\item[{float}]{temperature\+Threshold}{}\end{DoxyParamCaption})}



Sets board temperature threshold. 

\begin{DoxyReturn}{Returns}

\end{DoxyReturn}


Implemented in \mbox{\hyperlink{class_mr_e_module_sdk_1_1_devices_1_1_mre3_1_1_mr_e3_sdk_com_device_controller_a9b624903f9018b223bd6d091c98383bf}{Mr\+EModule\+Sdk.\+Devices.\+Mre3.\+Mr\+E3\+Sdk\+Com\+Device\+Controller}}.



The documentation for this interface was generated from the following file\+:\begin{DoxyCompactItemize}
\item 
C\+:/\+Users/jan.\+janda/\+Desktop/\+Mre3\+Documentation/\mbox{\hyperlink{_i_mre3_temperature_manager_8cs}{IMre3\+Temperature\+Manager.\+cs}}\end{DoxyCompactItemize}
