| optoMDC

Loading...
Searching...
No Matches
Public Member Functions | Static Public Member Functions | Public Attributes | Protected Attributes | List of all members
optoMDC.registers.mre3_registers.MRE3StaticInput Class Reference
Inheritance diagram for optoMDC.registers.mre3_registers.MRE3StaticInput:

## Public Member Functions
| __init__ (self, int channel=0, board=None)
| SetCurrent (self, value)
| GetCurrent (self)
| SetOF (self, value)
| GetOF (self)
| SetXY (self, value)
| GetXY (self)
| GetActiveType (self)

## Static Public Member Functions
| help ()

## Public Attributes
| sys_id
| current
| of
| xy_value
| active_type
| name

## Protected Attributes
| _readonly
| _channel

## Detailed Description

    Input Channel Systems - USB/UART
    System IDs: 0x50 through 0x57

    +----------------+------+-------------+----------+-------------+---------+---------------------------------------+
    | Register Name  | Id   | Type        | Unit     | Range       | Default | Comment                               |
    +================+======+=============+==========+=============+=========+=======================================+
    | current        | 0x00 | float 32-bit| A        | -0.7 to 0.7 | 0.0     |                                       |
    +----------------+------+-------------+----------+-------------+---------+---------------------------------------+
    | OF             | 0x00 | float 32-bit| A        |             | 0.0     |                                       |
    +----------------+------+-------------+----------+-------------+---------+---------------------------------------+
    | XY             | 0x00 | float 32-bit| A        | -1.0 to 1.0 | 0.0     |                                       |
    +----------------+------+-------------+----------+-------------+---------+---------------------------------------+
    | Type           | 0x00 | float 32-bit| A        |             | 0.0     |                                       |
    +----------------+------+-------------+----------+-------------+---------+---------------------------------------+
    | FP             | 0x00 | float 32-bit| A        |             | 0.0     |                                       |
    +----------------+------+-------------+----------+-------------+---------+---------------------------------------+
    | Unitless       | 0x00 | float 32-bit| A        |             | 0.0     |                                       |
    +----------------+------+-------------+----------+-------------+---------+---------------------------------------+

## Constructor & Destructor Documentation

## ◆ __init__()

optoMDC.registers.mre3_registers.MRE3StaticInput.__init__ | ( |  | self,
|  | int | channel = 0,
|  |  | board = None )

## Member Function Documentation

## ◆ GetActiveType()

optoMDC.registers.mre3_registers.MRE3StaticInput.GetActiveType | ( |  | self | ) |

## ◆ GetCurrent()

optoMDC.registers.mre3_registers.MRE3StaticInput.GetCurrent | ( |  | self | ) |

## ◆ GetOF()

optoMDC.registers.mre3_registers.MRE3StaticInput.GetOF | ( |  | self | ) |

## ◆ GetXY()

optoMDC.registers.mre3_registers.MRE3StaticInput.GetXY | ( |  | self | ) |

## ◆ help()

optoMDC.registers.mre3_registers.MRE3StaticInput.help | ( |  | ) |
| static

## ◆ SetCurrent()

optoMDC.registers.mre3_registers.MRE3StaticInput.SetCurrent | ( |  | self,
|  |  | value )

## ◆ SetOF()

optoMDC.registers.mre3_registers.MRE3StaticInput.SetOF | ( |  | self,
|  |  | value )

## ◆ SetXY()

optoMDC.registers.mre3_registers.MRE3StaticInput.SetXY | ( |  | self,
|  |  | value )

## Member Data Documentation

## ◆ _channel

optoMDC.registers.mre3_registers.MRE3StaticInput._channel
| protected

## ◆ _readonly

optoMDC.registers.mre3_registers.MRE3StaticInput._readonly
| protected

## ◆ active_type

optoMDC.registers.mre3_registers.MRE3StaticInput.active_type

## ◆ current

optoMDC.registers.mre3_registers.MRE3StaticInput.current

## ◆ name

optoMDC.registers.mre3_registers.MRE3StaticInput.name

## ◆ of

optoMDC.registers.mre3_registers.MRE3StaticInput.of

## ◆ sys_id

optoMDC.registers.mre3_registers.MRE3StaticInput.sys_id

## ◆ xy_value

optoMDC.registers.mre3_registers.MRE3StaticInput.xy_value

The documentation for this class was generated from the following file:

- C:/git/138-882-00_optoMDC/src/main/python/optoMDC/registers/mre3_registers.py