===================================================================================
   			Lens Driver Controller Release Notes
===================================================================================

Release Notes: 1.10 (133898-00-A)
-------------------------------------

[Added Features]
§ Updated driver installation help
§ Added firmaware Type F compatibility

[Resolved Bugs]
§ None

[Known Limitations]
§ None

[Reqiured User Actions]
§ None

[Compatibility]
§ Compatibility firmware
   - 1.8.X (133899-00-A)
   - 1.9.X (133899-00-A)
   - 1.9.X (133899-00-F)
§ Incompatible firmware
   - 1.3.X (133899-00-A)
   - 1.7.X (133899-00-A)


Release Notes: 1.9.5933 (133898-00-A)
-------------------------------------

[Added Features]
§ Updated driver installation help

[Resolved Bugs]
§ None

[Known Limitations]
§ None

[Required User Actions]
§ None

[Compatibility]
§ Compatibility firmware
  - Type A - 1.8.X / 1.9.X
  - Type F - 1.0.X
§ Incompatible firmware
  - Type A - 1.3.X / 1.7.X

Release Notes: 1.9.5765 (133898-00-A)
-------------------------------------

[Added Features]
§ Lens Driver Controller compatible to type F firmware 1.0.X

[Resolved Bugs]
§ Software does not crash when uEye framework is not installed and the user tries to open uEye viewer

[Known Limitations]
§ None

[Required User Actions]
§ None

[Compatibility]
§ Compatibility firmware
  - Type A - 1.8.X / 1.9.X
  - Type F - 1.0.X
§ Incompatible firmware
  - Type A - 1.3.X / 1.7.X


Release Notes 1.9.5722 (133898-00-A)
------------------------------------

[Added Features]
§ Framework extended to be compatible with upcoming firmware type releases
§ Signed Lens Driver driver included in the package
§ Ability to detect wether a connected Lens is compatible with the Lens Driver firmware
§ User is notified if outdated firmware on Lens Driver is detected
§ Incorporated "Expert Mode" into general user interface
§ Incorporated updated/new commands (see Lens Driver communication protocol definition)

[Resolved Bugs]
§ Software does not crash when uEye framework is not installed and the user tries to open uEye viewer

[Known Limitations]
§ None

[Required User Actions]
§ None

[Compatibility]
§ Compatible Firmware: 
  - Lens Driver V4 Firmware 1.8.X
  - Lens Driver V4 Firmware 1.9.X
§ Incompatible Firmware: 
  - Lens Driver V4 Firmware 1.3.X
  - Lens Driver V4 Firmware 1.7.X



Release Notes 1.8.5308.XXXXX
----------------------------

[Features]
§Backwards compatibility with Lens Driver firmware version 1.7.1147.XXXXX

[Fixed Bugs]
§uEye Camera Viewer notification panel fix.
§Serial ID error message bug fix.

[Known Limitations]
§Only fully tested for the EL-10-30-C  and El-6-18 lens 

[Compatibility]
§ Compatible Firmware: 
  - Lens Driver V4 Firmware 1.8.1230.XXXXX and up
§ Working Firmware: 
  - Lens Driver V4 Firmware 1.7.1149.XXXXX



Release Notes 1.8.5281.XXXXX
--------------------

[Features]
§ El-6-18 lens support
§ Firmware Analog mode is now available

[Fixed Bugs]
§ Sensor control mode only works after opening the lookup table window and closing it again.

[Known Limitations]
§ Only fully tested for the EL-10-30-C  and El-6-18 lens 

[Compatibility]
§ Compatible Firmware: 
  - Lens Driver V4 Firmware 1.8.1230.XXXXX and up



Release Notes 1.8.5199.XXXXX
--------------------

[Features]
§ Focal power sensor control has been re-enabled and improved.
§ DC mode sensor control has been implemented.
§ Creep compensation drift gain variable has been implemented with an accuracy of 0.01.
§ Improved error message readability.
§ Improved backwards compatibility (1.5 and up).
§ Toolstrip icon for enabled sensor control included.
§ Analop input "View" option included.
§ Updated software with the latest OptotuneComponent.
§ Rectangular, Sinusoidsal, and Triangular sessions are restored.

[Bug Fixes]
§ Analog input read fixed with latest firmware version.
§ Max current is now restricted to 0-655 mA in expert mode.
§ Focal power mode is now hidden if a lens with an empty/invalid EEPROM structure is connected.

[Known Limitations]
§ Only fully tested for the EL-10-30-C lens 

[Compatibility]
§ Compatible Firmware: 
  - Lens Driver V4 Firmware 1.7.1147.XXXXX and up
§ Outdated Firmware:
  - Lens Driver V4 Firmware 1.6.0.0 
  - Lens Driver V4 Firmware 1.5.0.0
§ Incompatible Firmware: 
  - Lens Driver V4 Firmware 1.3.0.0



Release Notes 1.8.5196.XXXXX
--------------------

[Features]
§ Bug Fixes from 1.8.5192.XXXXX

[Bug Fixes]
§ Deleting of rows in Sensor Control Configuration Form is more stable
§ Sensor Control Configuration Form does not constantly ask to save table when autofocusing in ueye viewer
§ Fixed interpolation error where only the first two calibration points were being used
§ Fixed error where it was needed to select "Sensor Control" twice

[Known Limitations]
§ Only fully tested for the EL-10-30-C lens 

[Compatibility]
§ Compatible Firmware: 
  - Lens Driver V4 Firmware 1.7.1140.57667 and up
§ Outdated Firmware:
  - Lens Driver V4 Firmware 1.6.0.0 
  - Lens Driver V4 Firmware 1.5.0.0
§ Incompatible Firmware: 
  - Lens Driver V4 Firmware 1.3.0.0



Release Notes 1.8.5192.XXXXX
--------------------

[Features]
§ Focal power sensor control has been re-enabled and improved.
§ DC mode sensor control has been implemented.
§ Creep compensation drift gain variable has been implemented with an accuracy of 0.01.
§ Improved error message readability.
§ Improved backwards compatibility (1.5 and up).
§ Toolstrip icon for enabled sensor control included.
§ Analop input "View" option included.
§ Updated software with the latest OptotuneComponent.
§ Rectangular, Sinusoidsal, and Triangular sessions are restored.

[Bug Fixes]
§ Analog input read fixed with latest firmware version.
§ Max current is now restricted to 0-655 mA in expert mode.
§ Focal power mode is now hidden if a lens with an empty/invalid EEPROM structure is connected.

[Known Limitations]
§ Only fully tested for the EL-10-30-C lens 

[Compatibility]
§ Compatible Firmware: 
  - Lens Driver V4 Firmware 1.7.1140.57667 and up
§ Outdated Firmware:
  - Lens Driver V4 Firmware 1.6.0.0 
  - Lens Driver V4 Firmware 1.5.0.0
§ Incompatible Firmware: 
  - Lens Driver V4 Firmware 1.3.0.0





