ICC-4c C# SDK

Public Member Functions | List of all members
ICC4cPwmSdk.Device.IEccTemperatureManager Interface Reference
Inheritance diagram for ICC4cPwmSdk.Device.IEccTemperatureManager:

## Public Member Functions
float | GetBoardOutputTemperature ()
| Returns board output temperature. More...
void | SetBoardOutputTemperatureThreshold (float temperatureThreshold)
| Sets board output temperature threshold. More...
float | GetBoardOutputTemperatureThreshold ()
| Returns board output temperature threshold. More...
float | GetBoardPowerTemperature ()
| Returns board power temperature. More...
void | SetBoardPowerTemperatureThreshold (float temperatureThreshold)
| Sets board power temperature threshold. More...
float | GetBoardPowerTemperatureThreshold ()
| Returns board power temperature threshold. More...
float | GetDeviceTemperature ()
| Returns device temperature. More...
void | SetDeviceTemperatureThreshold (float temperatureThreshold)
| Sets device temperature threshold. More...
float | GetDeviceTemperatureThreshold ()
| Returns board temperature threshold. More...

## Member Function Documentation

## ◆ GetBoardOutputTemperature()

float ICC4cPwmSdk.Device.IEccTemperatureManager.GetBoardOutputTemperature | ( |  | ) |

Returns board output temperature.

Returns

Implemented in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController.

## ◆ GetBoardOutputTemperatureThreshold()

float ICC4cPwmSdk.Device.IEccTemperatureManager.GetBoardOutputTemperatureThreshold | ( |  | ) |

Returns board output temperature threshold.

Returns

Implemented in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController.

## ◆ GetBoardPowerTemperature()

float ICC4cPwmSdk.Device.IEccTemperatureManager.GetBoardPowerTemperature | ( |  | ) |

Returns board power temperature.

Returns

Implemented in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController.

## ◆ GetBoardPowerTemperatureThreshold()

float ICC4cPwmSdk.Device.IEccTemperatureManager.GetBoardPowerTemperatureThreshold | ( |  | ) |

Returns board power temperature threshold.

Returns

Implemented in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController.

## ◆ GetDeviceTemperature()

float ICC4cPwmSdk.Device.IEccTemperatureManager.GetDeviceTemperature | ( |  | ) |

Returns device temperature.

Returns

Implemented in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController.

## ◆ GetDeviceTemperatureThreshold()

float ICC4cPwmSdk.Device.IEccTemperatureManager.GetDeviceTemperatureThreshold | ( |  | ) |

Returns board temperature threshold.

Returns

Implemented in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController.

## ◆ SetBoardOutputTemperatureThreshold()

void ICC4cPwmSdk.Device.IEccTemperatureManager.SetBoardOutputTemperatureThreshold | ( | float | temperatureThreshold | ) |

Sets board output temperature threshold.

Returns

Implemented in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController.

## ◆ SetBoardPowerTemperatureThreshold()

void ICC4cPwmSdk.Device.IEccTemperatureManager.SetBoardPowerTemperatureThreshold | ( | float | temperatureThreshold | ) |

Sets board power temperature threshold.

Returns

Implemented in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController.

## ◆ SetDeviceTemperatureThreshold()

void ICC4cPwmSdk.Device.IEccTemperatureManager.SetDeviceTemperatureThreshold | ( | float | temperatureThreshold | ) |

Sets device temperature threshold.

Returns

Implemented in ICC4cPwmSdk.Device.Ecc1cSdkDeviceController.

The documentation for this interface was generated from the following file:

- Device/Ecc1cSdkDeviceController.cs